# Linux* Base Driver for 10 Gigabit Intel® Network Connection

| NOTES: This release includes the ixgbe and ixgbevf Linux* Base Drivers for the Intel® 10 Gigabit Family of Adapters.
| All 82599 and 82598-based 10 Gigabit network connections require the ixgbe driver. The ixgbevf driver supports 82599-based virtual function devices that can only be activated on kernels that support SR-IOV. SR-IOV requires the correct platform and OS support.

# Using the ixgbe base driver

Important Note

Overview

Building and Installation

Command Line Parameters

Additional Configurations

Performance Tuning

Known Issues/Troubleshooting

## Important Note

| Warning: The ixgbe driver compiles by default with the LRO (Large Receive Offload) feature enabled. This option offers the lowest CPU utilization for receives, but is completely incompatible with *routing/ip forwarding* and *bridging*. If enabling ip forwarding or bridging is a requirement, it is necessary to disable LRO using compile time options as noted in the LRO section later in this document. The result of not disabling LRO when combined with ip forwarding or bridging can be low throughput or even a kernel PANIC.

## Overview

The Linux* base driver supports the 2.6.x kernel, and includes support for any Linux supported system, including Itanium(R)2, x86_64, i686, and PPC.
These drivers are only supported as a loadable module at this time. Intel is not supplying patches against the kernel source to allow for static linking of the driver. A version of the driver may already be included by your distribution and/or the kernel.org kernel. For questions related to hardware requirements, refer to the documentation supplied with your Intel adapter. All hardware requirements listed apply to use with Linux.
The following features are now available in supported kernels:

- Native VLANs

- Channel Bonding (teaming)

- SNMP

- Generic Receive Offload

- Data Center Bridging

Channel Bonding documentation can be found in the Linux kernel source: /Documentation/networking/bonding.txt

The driver information previously displayed in the /proc file system is not supported in this release. Alternatively, you can use ethtool (version 1.6 or later), lspci, and ifconfig to obtain the same information. Instructions on updating ethtool can be found in the section Additional Configurations later in this document.

The driver in this release is compatible with 82598 and 82599-based Intel Network Connections.

For more information on how to identify your adapter, go to the Adapter & Driver ID Guide at:

> http://support.intel.com/support/go/network/adapter/proidguide.htm

For the latest Intel network drivers for Linux, refer to the following website. Select the link for your adapter.

> http://support.intel.com/support/go/network/adapter/home.htm

### SFP+ Devices with Pluggable Optics

#### 82599-BASED ADAPTERS

| NOTES: If your 82599-based Intel® Network Adapter came with Intel optics or is an Intel® Ethernet Server Adapter X520-2, then it only supports Intel optics and/or the direct attach cables listed below. When 82599-based SFP+ devices are connected back to back, they should be set to the same Speed setting via ethtool. Results may vary if you mix speed settings.

Supplier | Type | Part Numbers
SR Modules |  |
Intel | DUAL RATE 1G/10G SFP+ SR (bailed) | AFBR-703SDZ-IN2
Intel | DUAL RATE 1G/10G SFP+ SR (bailed) | FTLX8571D3BCV-IT
Intel | DUAL RATE 1G/10G SFP+ SR (bailed) | AFBR-703SDDZ-IN1
LR Modules |  |
Intel | DUAL RATE 1G/10G SFP+ LR (bailed) | FTLX1471D3BCV-IT
Intel | DUAL RATE 1G/10G SFP+ LR (bailed) | AFCT-701SDZ-IN2
Intel | DUAL RATE 1G/10G SFP+ LR (bailed) | AFCT-701SDDZ-IN1

The following is a list of 3rd party SFP+ modules and direct attach cables that have received some testing. Not all modules are applicable to all devices.

Supplier | Type | Part Numbers
Finisar | SFP+ SR bailed, 10g single rate | FTLX8571D3BCL
Avago | SFP+ SR bailed, 10g single rate | AFBR-700SDZ
Finisar | SFP+ LR bailed, 10g single rate | FTLX1471D3BCL
Finisar | DUAL RATE 1G/10G SFP+ SR (No Bail) | FTLX8571D3QCV-IT
Avago | DUAL RATE 1G/10G SFP+ SR (No Bail) | AFBR-703SDZ-IN1
Finisar | DUAL RATE 1G/10G SFP+ LR (No Bail) | FTLX1471D3QCV-IT
Avago | DUAL RATE 1G/10G SFP+ LR (No Bail) | AFCT-701SDZ-IN1
Finisar | 1000BASE-T SFP | FCLF8522P2BTL
Avago | 1000BASE-T SFP | ABCU-5710RZ

82599-based adapters support all passive and active limiting direct attach cables that comply with SFF-8431 v4.1 and SFF-8472 v10.4 specifications.

#### Laser turns off for SFP+ when ifconfig down

"ifconfig down" turns off the laser for 82599-based SFP+ fiber adapters. "ifconfig up" turns on the laser.

#### 82598-BASED ADAPTERS

| NOTES: Intel® Network Adapters that support removable optical modules only support their original module type (i.e., the Intel® 10 Gigabit SR Dual Port Express Module only supports SR optical modules). If you plug in a different type of module, the driver will not load. Hot Swapping/hot plugging optical modules is not supported. Only single speed, 10 gigabit modules are supported. LAN on Motherboard (LOMs) may support DA, SR, or LR modules. Other module types are not supported. Please see your system documentation for details.

The following is a list of SFP+ modules and direct attach cables that have received some testing. Not all modules are applicable to all devices.

Supplier | Type | Part Numbers
Finisar | SFP+ SR bailed, 10g single rate | FTLX8571D3BCL
Avago | SFP+ SR bailed, 10g single rate | AFBR-700SDZ
Finisar | SFP+ LR bailed, 10g single rate | FTLX1471D3BCL

82598-based adapters support all passive direct attach cables that comply with SFF-8431 v4.1 and SFF-8472 v10.4 specifications. Active direct attach cables are not supported.

THIRD PARTY OPTIC MODULES AND CABLES REFERRED TO ABOVE ARE LISTED ONLY FOR THE PURPOSE OF HIGHLIGHTING THIRD PARTY SPECIFICATIONS AND POTENTIAL COMPATIBILITY, AND ARE NOT RECOMMENDATIONS OR ENDORSEMENT OR SPONSORSHIP OF ANY THIRD PARTY’S PRODUCT BY INTEL. INTEL IS NOT ENDORSING OR PROMOTING PRODUCTS MADE BY ANY THIRD PARTY AND THE THIRD PARTY REFERENCE IS PROVIDED ONLY TO SHARE INFORMATION REGARDING CERTAIN OPTIC MODULES AND CABLES WITH THE ABOVE SPECIFICATIONS. THERE MAY BE OTHER MANUFACTURERS OR SUPPLIERS, PRODUCING OR SUPPLYING OPTIC MODULES AND CABLES WITH SIMILAR OR MATCHING DESCRIPTIONS. CUSTOMERS MUST USE THEIR OWN DISCRETION AND DILIGENCE TO PURCHASE OPTIC MODULES AND CABLES FROM ANY THIRD PARTY OF THEIR CHOICE. CUSTOMERS ARE SOLELY RESPONSIBLE FOR ASSESSING THE SUITABILITY OF THE PRODUCT AND/OR DEVICES AND FOR THE SELECTION OF THE VENDOR FOR PURCHASING ANY PRODUCT. THE OPTIC MODULES AND CABLES REFERRED TO ABOVE ARE NOT WARRANTED OR SUPPORTED BY INTEL. INTEL ASSUMES NO LIABILITY WHATSOEVER, AND INTEL DISCLAIMS ANY EXPRESS OR IMPLIED WARRANTY, RELATING TO SALE AND/OR USE OF SUCH THIRD PARTY PRODUCTS OR SELECTION OF VENDOR BY CUSTOMERS.

## Building and Installation

To build a binary RPM* package of this driver, run 'rpmbuild -tb ixgbe.tar.gz'.

| NOTE: For the build to work properly, the currently running kernel MUST match the version and configuration of the installed kernel sources. If you have just recompiled the kernel reboot the system now. RPM functionality has only been tested in Red Hat distributions.

To manually build this driver:

1. Move the base driver tar file to the directory of your choice. For example, use '/home/username/ixgbe' or '/usr/local/src/ixgbe'.

2. Untar/unzip the archive:

   > tar zxf ixgbe-x.x.x.tar.gz

3. Change to the driver src directory:

   > cd ixgbe-x.x.x/src/

4. Compile the driver module:

   > make install

   The binary will be installed as:

   > /lib/modules/[KERNEL_VERSION]/kernel/drivers/net/ixgbe/ixgbe.[k]o

   The install location listed above is the default location. This may differ for various Linux distributions.

5. Load the module:
   For kernel 2.6.x, use the modprobe command -

   modprobe ixgbe <parameter>=<value>

   Note that for 2.6 kernels the insmod command can be used if the full path to the driver module is specified. For example:
   insmod /lib/modules/<KERNEL VERSION>/kernel/drivers/net/ixgbe/ixgbe.ko

   With 2.6 based kernels also make sure that older ixgbe drivers are removed from the kernel, before loading the new module:

   > rmmod ixgbe; modprobe ixgbe

6. Assign an IP address to the interface by entering the following, where x is the interface number:

   > ifconfig ethx <IP_address> netmask <netmask>

7. Verify that the interface works. Enter the following, where <IP_address> is the IP address of another machine on the same subnet as the interface that is being tested:

   > ping <IP_address>

### To build ixgbe driver with DCA

If your kernel supports DCA, the driver will build by default with DCA enabled.

## Command Line Parameters

If the driver is built as a module, the following optional parameters are used by entering them on the command line with the modprobe command using this syntax:

> modprobe ixgbe [<option>=<VAL1>,<VAL2>,...]

For example:

> modprobe ixgbe InterruptThrottleRate=16000,16000

The default value for each parameter is generally the recommended setting, unless otherwise noted.

Parameter Name | Valid Range/Settings | Default | Description
--- | --- | --- | ---
RSS - Receive Side Scaling (or multiple queues for receives) | 0 - 16 | 1 | 0 = disables RSS 1 = enables RSS and sets the descriptor queue count to 16 or the number of online cpus, whichever is less. 2-16 = enables RSS, with 2-16 queues RSS also effects the number of transmit queues allocated on 2.6.23 and newer kernels with CONFIG_NETDEVICES_MULTIQUEUE set in the kernel .config file. CONFIG_NETDEVICES_MULTIQUEUE only exists from 2.6.23 to 2.6.26. Other options enable multiqueue in 2.6.27 and newer kernels.
| NOTE: The RSS parameter has no effect on 82599-based adapters unless the FdirMode parameter is simultaneously used to disable Flow Director. See Intel(R) Ethernet Flow Director section for more detail.
MQ - Multi Queue | 0, 1 | 1 | 0 = Disables Multiple Queue support 1 = Enabled Multiple Queue support (a prerequisite for RSS)
DCA - Direct Cache Access | 0, 1 | 1 (when IXGBE_DCA is enabled) | 0 = Disables DCA support in the driver 1 = Enables DCA support in the driver See the above instructions for enabling DCA. If the driver is enabled for DCA this parameter allows load-time control of the feature.
RxBufferMode | 0-2 | 2 (82598-based adapters) 0 (82599-based adapters) | 0 = Driver will use single buffer for Rx packets. 1 = Driver will use packet split mode for Rx. Packet header will be received in header buffer and payload will be received in data buffer. 2. = Optimal mode. Driver will use single buffer mode for non-Jumbo configurations and packet split mode for Jumbo configurations.
| NOTE: HeaderDataSplit is not supported in 82599-based adapters.
IntMode | 0-2 (0 = Legacy Int, 1 = MSI and 2 = MSIX) | 2 | IntMode controls allow load time control over the type of interrupt registered for by the driver. MSI-X is required for multiple queue support, and some kernels and combinations of kernel .config options will force a lower level of interrupt support. 'cat /proc/interrupts' will show different values for each type of interrupt.
InterruptThrottleRate | 956-488281 (0=off, 1=dynamic) | 1 | Interrupt Throttle Rate (interrupts/sec). The ITR parameter controls how many interrupts each interrupt vector can generate per second. Increasing ITR lowers latency at the cost of increased CPU utilization, though it may help throughput in some circumstances. 1 = Dynamic mode attempts to moderate interrupts per vector while maintaining very low latency. This can sometimes cause extra CPU utilization. If planning on deploying ixgbe in a latency sensitive environment please consider this parameter. 0 = Setting InterruptThrottleRate to 0 turns off any interrupt moderation and may improve small packet latency, but is generally not suitable for bulk throughput traffic due to the increased cpu utilization of the higher interrupt rate. Please note that on 82599-based adapters, disabling InterruptThrottleRate will also result in the driver disabling HW RSC. On 82598-based adapters, disabling InterruptThrottleRate will also result in disabling LRO (Large Receive Offloads).
LLI (Low Latency Interrupts) |  |  | LLI allows for immediate generation of an interrupt upon processing receive packets that match certain criteria as set by the parameters described below. LLI parameters are not enabled when Legacy interrupts are used. You must be using MSI or MSI-X (see cat /proc/interrupts) to successfully use LLI.
LLIPort | 0 - 65535 | 0 (disabled) | LLI is configured with the LLIPort command-line parameter, which specifies which TCP port should generate Low Latency Interrupts. For example, using LLIPort=80 would cause the hardware to generate an immediate interrupt upon receipt of any packet sent to TCP port 80 on the local machine.
| CAUTION: Enabling LLI can result in an excessive number of interrupts/second that may cause problems with the system and in some cases may cause a kernel panic.
LLIPush | 0-1 | 0 (disabled) | LLIPush can be set to be enabled or disabled (default). It is most effective in an environment with many small transactions. NOTE: Enabling LLIPush may allow a denial of service attack.
LLISize | 0-1500 | 0 (disabled) | LLISize causes an immediate interrupt if the board receives a packet smaller than the specified size.
LLIEType | 0-x8fff | 0 (disabled) | Low Latency Interrupt Ethernet Protocol Type.
LLIVLANP | 0-7 | 0 (disabled) | Low Latency Interrupt on VLAN priority threshold.
Flow Control |  |  | Ethernet Flow Control (IEEE 802.3x) can be configured with ethtool to enable receiving and transmitting pause frames for ixgbe. When tx is enabled, PAUSE frames are generated when the receive packet buffer crosses a predefined threshold. When rx is enabled, the transmit unit will halt for the time delay specified when a PAUSE frame is received. Flow Control is enabled by default. If you want to disable a flow control capable link partner, use ethtool: ethtool -A eth? autoneg off rx off tx off
| NOTE: For 82598 backplane cards entering 1 gig mode, flow control default behavior is changed to off. Flow control in 1 gig mode on these devices can lead to Tx hangs.
Intel® Ethernet Flow Director |  |  | Supports advanced filters that direct receive packets by their flows to different queues. Enables tight control on routing a flow in the platform. Matches flows and CPU cores for flow affinity. Supports multiple parameters for flexible flow classification and load balancing. Flow director is enabled only if the kernel is multiple TX queue capable. An included script (set_irq_affinity.sh) automates setting the IRQ to CPU affinity. You can verify that the driver is using Flow Director by looking at the counter in ethtool: fdir_miss and fdir_match. Other ethtool Commands: To enable Flow Director ethtool -K ethX ntuple on To add a filter Use -U switch. e.g., ethtool -U ethX flow-type tcp4 src-ip 0x178000a action 1 To see the list of filters currently present: ethtool -u ethX Perfect Filter: Perfect filter is an interface to load the filter table that funnels all flow into queue_0 unless an alternative queue is specified using "action". In that case, any flow that matches the filter criteria will be directed to the appropriate queue. If the queue is defined as -1, filter will drop matching packets. To account for filter matches and misses, there are two stats in ethtool: fdir_match and fdir_miss. In addition, rx_queue_N_packets shows the number of packets processed by the Nth queue.
| NOTE: Receive Packet Steering (RPS) and Receive Flow Steering (RFS) are not compatible with Flow Director. IF Flow Director is enabled, these will be disabled.
The following three parameters impact Flow Director.
FdirMode | 0-2 (0=off, 1=ATR, 2=Perfect filter mode) | 1 (ATR) | Flow Director filtering modes.
FdirPballoc | 0-2 (0=64k, 1=128k, 2=256k) | 0 (64k) | Flow Director allocated packet buffer size.
AtrSampleRate | 1-100 | 20 | Software ATR Tx packet sample rate. For example, when set to 20, every 20th packet, looks to see if the packet will create a new flow.
max_vfs | 1-63 | 0 | If the value is greater than 0 it will also force the VMDq parameter to be 1 or more. This parameter adds support for SR-IOV. It causes the driver to spawn up to max_vfs worth of virtual function. The parameters for the driver are referenced by position. So, if you have a dual port 82599-based adapter and you want N virtual functions per port, you must specify a number for each port with each parameter separated by a comma. For example: insmod ixgbe max_vfs=63,63
| NOTE: If both 82598 and 82599-based adapters are installed on the same machine, you must be careful in loading the driver with the parameters. Depending on system configuration, number of slots, etc. it’s impossible to predict in all cases where the positions would be on the command line and the user will have to specify zero in those positions occupied by an 82598 port.
Node | 0-n | 1 (off) | The Node parameter will allow you to pick which NUMA node you want to have the adapter allocate memory on. 0 – n: where n is the number of NUMA nodes (i.e. 0 – 3) currently online in your system. 1: turns this option off
L2LBen | 0 = disable, 1 = enable (default) | 1 (enable) | This parameter controls the internal switch (L2 loopback between pf and vf). By default the switch is enabled.

## Additional Configurations

### Configuring the Driver on Different Distributions

Configuring a network driver to load properly when the system is started is distribution dependent. Typically, the configuration process involves adding an alias line to /etc/modules.conf or etc/modprobe.conf, as well as editing other system startup scripts and/or configuration files. Many popular Linux distributions ship with tools to make these changes for you. To learn the proper way to configure a network device for your system, refer to your distribution documentation. If during this process you are asked for the driver or module name, the name for the Linux Base Driver for the 10 Gigabit Family of Adapters is ixgbe.

### Viewing Link Messages

Link messages will not be displayed to the console if the distribution is restricting system messages. In order to see network driver link messages on your console, set dmesg to eight by entering the following:

dmesg -n 8

| NOTE: This setting is not saved across reboots.

### Jumbo Frames

The driver supports Jumbo Frames for all adapters. Jumbo Frames support is enabled by changing the MTU to a value larger than the default of 1500. The maximum value for the MTU is 16110. Use the ifconfig command to increase the MTU size. For example, enter the following where <x> is the interface number:

> ifconfig ethx mtu 9000 up

The maximum MTU setting for Jumbo Frames is 16110. This value coincides with the maximum Jumbo Frames size of 16128. This driver will attempt to
use multiple page sized buffers to receive each jumbo packet. This should help to avoid buffer starvation issues when allocating receive packets.

### ethtool

The driver utilizes the ethtool interface for driver configuration and diagnostics, as well as displaying statistical information. The latest ethtool version is required for this functionality.

The latest release of ethtool can be found at: http://ftp.kernel.org/pub/software/network/ethtool/.

### NAPI

NAPI (Rx polling mode) is supported in the ixgbe driver. NAPI is enabled or disabled based on the configuration of the kernel. To override the default, use the following compile-time flags.

You can tell if NAPI is enabled in the driver by looking at the version number of the driver. It will contain the string -NAPI if NAPI is enabled.

To enable NAPI, compile the driver module, passing in a configuration option:

make CFLAGS_EXTRA=-DIXGBE_NAPI install

| NOTE: This will not do anything if NAPI is disabled in the kernel.

To disable NAPI, compile the driver module, passing in a configuration option:
make CFLAGS_EXTRA=-DIXGBE_NO_NAPI install

See www.cyberus.ca/~hadi/usenix-paper.tgz for more information on NAPI.

### LRO

Large Receive Offload (LRO) is a technique for increasing inbound throughput of high-bandwidth network connections by reducing CPU overhead. It works by aggregating multiple incoming packets from a single stream into a larger buffer before they are passed higher up the networking stack, thus reducing the number of packets that have to be processed. LRO combines multiple Ethernet frames into a single receive in the stack, thereby potentially decreasing CPU utilization for receives.

IXGBE_NO_LRO is a compile time flag. The user can enable it at compile time to remove support for LRO from the driver. The flag is used by adding
CFLAGS_EXTRA="-DIXGBE_NO_LRO" to the make file when it's being compiled.

> make CFLAGS_EXTRA="-DIXGBE_NO_LRO" install

You can verify that the driver is using LRO by looking at these counters in ethtool:

> lro_flushed - the total number of receives using LRO.

> lro_aggregated - counts the total number of Ethernet packets that were combined.

| NOTE: IPv6 and UDP are not supported by LRO.

### HW RSC

82599-based adapters support HW based receive side coalescing (RSC) which can merge multiple frames from the same IPv4 TCP/IP flow into a single structure that can span one or more descriptors. It works similarly to SW Large receive offload technique. By default HW RSC is enabled and SW LRO can not be used for 82599-based adapters unless HW RSC is disabled.
IXGBE_NO_HW_RSC is a compile time flag. The user can enable it at compile time to remove support for HW RSC from the driver. The flag is used by adding CFLAGS_EXTRA="-DIXGBE_NO_HW_RSC" to the make file when it's being compiled.

make CFLAGS_EXTRA="-DIXGBE_NO_HW_RSC" install

You can verify that the driver is using HW RSC by looking at the counter in ethtool:

hw_rsc_count - counts the total number of Ethernet packets that were being combined.

### rx_dropped_backlog

When in a non-Napi (or Interrupt) mode, this counter indicates that the stack is dropping packets. There is an adjustable parameter in the stack that allows you to adjust the amount of backlog. We recommend increasing the netdev_max_backlog if the counter goes up.

> # sysctl -a |grep netdev_max_backlog

> net.core.netdev_max_backlog = 1000

> # sysctl -e net.core.netdev_max_backlog=10000

> net.core.netdev_max_backlog = 10000

### Flow Control

Flow control is enabled by default. If you want to disable a flow control capable link partner, use ethtool:
ethtool -A eth? autoneg off rx off tx off

### MAC and VLAN anti-spoofing feature

When a malicious driver attempts to send a spoofed packet, it is dropped by the hardware and not transmitted. An interrupt is sent to the PF driver notifying it of the spoof attempt.
When a spoofed packet is detected the PF driver will send the following message to the system log (displayed by the "dmesg" command):

> ixgbe ethx: ixgbe_spoof_check: n spoofed packets detected
> Where x=the PF interface# n=the VF that attempted to do the spoofing.

## Performance Tuning

An excellent article on performance tuning can be found at:

http://www.redhat.com/promo/summit/2008/downloads/pdf/Thursday/Mark_Wagner.pdf

## Known Issues/Troubleshooting

| NOTE: After installing the driver, if your Intel Network Connection is not working, verify that you have installed the correct driver.

### MSI-X Issues with Kernels between 2.6.19 - 2.6.21 (inclusive)

Kernel panics and instability may be observed on any MSI-X hardware if you use irqbalance with kernels between 2.6.19 and 2.6.21. If such problems are encountered, you may disable the irqbalance daemon or upgrade to a newer kernel.

### Driver Compilation

When trying to compile the driver by running make install, the following error may occur: "Linux kernel source not configured - missing version.h"

To solve this issue, create the version.h file by going to the Linux source tree and entering:

> make include/linux/version.h

### Do Not Use LRO When Routing or Bridging Packets

Due to a known general compatibility issue with LRO and routing, do not use LRO when routing or bridging packets.

### LRO and iSCSI Incompatibility

LRO is incompatible with iSCSI target or initiator traffic. A panic may occur when iSCSI traffic is received through the ixgbe driver with LRO enabled. To workaround this, the driver should be built and installed with:

> # make CFLAGS_EXTRA=-DIXGBE_NO_LRO install

### Performance Degradation with Jumbo Frames

Degradation in throughput performance may be observed in some Jumbo frames environments. If this is observed, increasing the application's socket buffer size and/or increasing the /proc/sys/net/ipv4/tcp_*mem entry values may help. See the specific application manual and /usr/src/linux*/Documentation/networking/ip-sysctl.txt for more details.

### Multiple Interfaces on Same Ethernet Broadcast Network

Due to the ARP behavior on Linux, it is not possible to have one system on two IP networks in the same Ethernet broadcast domain (non-partitioned switch) behave as expected. All Ethernet interfaces will respond to IP traffic for any IP address assigned to the system. This results in unbalanced receive traffic.

If you have multiple interfaces in a server, either turn on ARP filtering by entering:

echo 1 > /proc/sys/net/ipv4/conf/all/arp_filter

(this only works if your kernel's version is higher than 2.4.5), or install the interfaces in separate broadcast domains (either in different switches or in a switch partitioned to VLANs).

### UDP Stress Test Dropped Packet Issue

Under small packets UDP stress test with 10GbE driver, the Linux system may drop UDP packets due to the fullness of socket buffers. You may want to change the driver's Flow Control variables to the minimum value for controlling packet reception.

Or you can increase the kernel's default buffer sizes for UDP by changing the values in

> /proc/sys/net/core/rmem_default and rmem_max

### Unplugging network cable while ethtool -p is running

In kernel versions 2.5.50 and later (including 2.6 kernel), unplugging the network cable while ethtool -p is running will cause the system to become unresponsive to keyboard commands, except for control-alt-delete. Restarting the system appears to be the only remedy.

### Cisco Catalyst 4948-10GE port resets may cause switch to shut down ports

82598-based hardware can re-establish link quickly and when connected to some switches, rapid resets within the driver may cause the switch port to become
isolated due to "link flap". This is typically indicated by a yellow instead of a green link light. Several operations may cause this problem, such as repeatedly running ethtool commands that cause a reset.
A potential workaround is to use the Cisco IOS command "no errdisable detect cause all" from the Global Configuration prompt which enables the switch to keep the interfaces up, regardless of errors.

### Installing Red Hat Enterprise Linux 4.7, 5.1, or 5.2 with an Intel(R) 10 Gigabit AT Server Adapter may cause kernel panic

A known issue may cause a kernel panic or hang after installing an 82598AT-based Intel(R) 10 Gigabit AT Server Adapter in a Red Hat Enterprise Linux 4.7, 5.1, or 5.2 system. The ixgbe driver for both the install kernel and the runtime kernel can create this panic if the 82598AT adapter is installed. Red Hat may release a security update that contains a fix for the panic that you can download using RHN (Red Hat Network) or Intel recommends that you install the ixgbe-1.3.31.5 driver or newer BEFORE installing the hardware.

### Rx Page Allocation Errors

Page allocation failure. order:0 errors may occur under stress with kernels 2.6.25 and above. This is caused by the way the Linux kernel reports this stressed condition.

### DCB: Generic segmentation offload on causes bandwidth allocation issues

In order for DCB to work correctly, GSO (Generic Segmentation Offload aka software TSO) must be disabled using ethtool. By default since the hardware supports TSO (hardware offload of segmentation) GSO will not be running. The GSO state can be queried with ethtool using ethtool -k ethX.

### When using 82598-based network connections, ixgbe driver only supports 16 queues on a platform with more than 16 cores

Due to known hardware limitations, RSS can only filter in a maximum of 16 receive queues.
82599-based network connections support up to 64 queues.

### Disable GRO when routing/bridging

Due to a known kernel issue, GRO must be turned off when routing/bridging. GRO can be turned off via ethtool.

ethtool -K ethX gro off
where ethX is the ethernet interface you're trying to modify.

### Lower than expected performance on dual port 10GbE devices

Some PCI-E x8 slots are actually configured as x4 slots. These slots have insufficient bandwidth for full 10Gbe line rate with dual port 10GbE devices. The driver can detect this situation and will write the following message in the system log: “PCI-Express bandwidth available for this card is not sufficient for optimal performance. For optimal performance a x8 PCI-Express slot is required.”

If this error occurs, moving your adapter to a true x8 slot will resolve the issue.

### ethtool may incorrectly display SFP+ fiber module as Direct Attached cable

Due to kernel limitations, port type can only be correctly displayed on kernel 2.6.33 or greater.

### Under Redhat 5.4 - System May Crash when Closing Guest OS Window after Loading/Unloading Physical Function (PF) Driver

Do not remove the ixgbe driver from Dom0 while Virtual Functions (VFs) are assigned to guests. VFs must first use the xm "pci-detach" command to hot-plug the VF device out of the VM it is assigned to or else shut down the VM.

### Unloading Physical Function (PF) Driver Causes System Reboots When VM is Running and VF is Loaded on the VM

Do not unload the PF driver (ixgbe) while VFs are assigned to guests.

### Running ethtool -t ethX command causes break between PF and test client

When there are active VFs, "ethtool -t" will only run the link test. The driver will also log in syslog that VFs should be shut down to run a full diags test.

### SLES10 SP3 random system panic when reloading driver

This is a known SLES-10 SP3 issue. After requesting interrupts for MSI-X vectors, system may panic.

Currently the only known workaround is to build the drivers with CFLAGS_EXTRA=-DDISABLE_PCI_MSI if the driver need to be loaded/unloaded. Otherwise the driver can be loaded once and will be safe, but unloading it will lead to the issue.

### Enabling SR-IOV in a 32-bit or 64-bit Microsoft* Windows* Server 2008/R2 Guest OS using Intel® 82576-based GbE or Intel® 82599-based 10GbE controller under KVM

KVM Hypervisor/VMM supports direct assignment of a PCIe device to a VM. This includes traditional PCIe devices, as well as SR-IOV-capable devices using Intel 82576-based and 82599-based controllers.
While direct assignment of a PCIe device or an SR-IOV Virtual Function (VF) to a Linux-based VM running 2.6.32 or later kernel works fine, there is a known issue with Microsoft Windows Server 2008/R2 VM that results in a "yellow bang" error. This problem is within the KVM VMM itself, not the Intel driver, or the SR-IOV logic of the VMM, but rather that KVM emulates an older CPU model for the guests, and this older CPU model does not support MSI-X interrupts, which is a requirement for Intel SR-IOV.
If you wish to use the Intel 82576 or 82599-based controllers in SR-IOV mode with KVM and a Microsoft Windows Server 2008/R2 guest try the following workaround. The workaround is to tell KVM to emulate a different model of CPU when using qemu to create the KVM guest:

> "-cpu qemu64,model=13"

## Support

For general information, go to the Intel support website at:

www.intel.com/support/

If an issue is identified with the released source code on the supported kernel with a supported adapter, email the specific information related to the issue to linux.nics@intel.com.

# Using the ixgbevf Base Driver

Overview

Building and Installation

Command Line Parameters

Additional Configurations

Known Issues

## Overview

This driver supports upstream kernel versions 2.6.30 (or higher) x86_64.

Supported Operating Systems: SLES 11 SP1 x86_64, RHEL 5.3/5.4 x86_64.
The ixgbevf driver supports 82599-based virtual function devices that can only be activated on kernels that support SR-IOV. SR-IOV requires the correct platform and OS support.
The ixgbevf driver requires the ixgbe driver, version 2.0 or later. The ixgbevf driver supports virtual functions generated by the ixgbe driver with a max_vfs value of 1 or greater. For more information on the max_vfs parameter refer to the section on the the ixgbe driver.

The guest OS loading the ixgbevf driver must support MSI-X interrupts.
This driver is only supported as a loadable module at this time. Intel is not supplying patches against the kernel source to allow for static linking of the driver. For questions related to hardware requirements, refer to the documentation supplied with your Intel Gigabit adapter. All hardware requirements listed apply to use with Linux.
Instructions on updating ethtool can be found in the section Additional Configurations later in this document.
VLANs: There is a limit of a total of 64 shared VLANs to 1 or more VFs.

## Building and Installation

To build a binary RPM* package of this driver, run 'rpmbuild -tb <filename.tar.gz>'. Replace <filename.tar.gz> with the specific filename of the driver.

| NOTE: For the build to work properly, the currently running kernel MUST match the version and configuration of the installed kernel sources. If you have just recompiled the kernel reboot the system now.

RPM functionality has only been tested in Red Hat distributions.

1. Move the base driver tar file to the directory of your choice. For example, use ' /home/username/ ixgbevf or /usr/local/src/ ixgbevf.'.

2. Untar/unzip the archive:

   > tar zxf ixgbevf-x.x.x.tar.gz

3. Change to the driver src directory:

   > cd ixgbevf-<x.x.x>/src/

4. Compile the driver module:

   > # make install

   The binary will be installed as:

   > /lib/modules/<KERNEL VERSION>/kernel/drivers/net/ixgbevf/ixgbevf.[k]o

   The install location listed above is the default location. This may differ for various Linux distributions.

5. Load the module using either the insmod or modprobe command:

   > modprobe ixgbevf

   > insmod ixgbevf

   Note that for 2.6 kernels the insmod command can be used if the full path to the driver module is specified. For example:

   insmod /lib/modules/<KERNEL VERSION>/kernel/drivers/net/ixgbevf/ixgbevf.ko

   With 2.6 based kernels also make sure that older e1000e drivers are removed from the kernel, before loading the new module:

   > rmmod ixgbevf; modprobe ixgbevf

6. Assign an IP address to the interface by entering the following, where <x> is the interface number:

   > ifconfig eth<x> <IP_address>

7. Verify that the interface works. Enter the following, where <IP_address> is the IP address for another machine on the same subnet as the interface that is being tested:

   > ping <IP_address>

## Command Line Parameters

If the driver is built as a module, the following optional parameters are used by entering them on the command line with the modprobe command using this syntax:

> modprobe ixgbevf [<option>=<VAL1>,<VAL2>,...]

For example:

> modprobe ixgbevf InterruptThrottleRate=16000,16000

The default value for each parameter is generally the recommended setting, unless otherwise noted.

| NOTES: For more information about the InterruptThrottleRate parameter, see the application note at: http://www.intel.com/design/network/applnots/ap450.htm. A descriptor describes a data buffer and attributes related to the data buffer. This information is accessed by the hardware.

Parameter Name | Valid Range/Settings | Default | Description
--- | --- | --- | ---
InterruptThrottleRate | 0,1,956-488281 (0=off, 1=dynamic) | 8000 | The driver can limit the amount of interrupts per second that the adapter will generate for incoming packets. It does this by writing a value to the adapter that is based on the maximum amount of interrupts that the adapter will generate per second. Setting InterruptThrottleRate to a value greater or equal to 100 will program the adapter to send out a maximum of that many interrupts per second, even if more packets have come in. This reduces interrupt load on the system and can lower CPU utilization under heavy load, but will increase latency as packets are not processed as quickly. The default behaviour of the driver previously assumed a static InterruptThrottleRate value of 8000, providing a good fallback value for all traffic types, but lacking in small packet performance and latency. The hardware can handle many more small packets per second however, and for this reason an adaptive interrupt moderation algorithm was implemented. The driver has one adaptive mode (setting 1) in which it dynamically adjusts the InterruptThrottleRate value based on the traffic that it receives. After determining the type of incoming traffic in the last timeframe, it will adjust the InterruptThrottleRate to an appropriate value for that traffic. The algorithm classifies the incoming traffic every interval into classes. Once the class is determined, the InterruptThrottleRate value is adjusted to suit that traffic type the best. There are three classes defined: "Bulk traffic", for large amounts of packets of normal size; "Low latency", for small amounts of traffic and/or a significant percentage of small packets; and "Lowest latency", for almost completely small packets or minimal traffic. In dynamic conservative mode, the InterruptThrottleRate value is set to 4000 for traffic that falls in class "Bulk traffic". If traffic falls in the "Low latency" or "Lowest latency" class, the InterruptThrottleRate is increased stepwise to 20000. This default mode is suitable for most applications. For situations where low latency is vital such as cluster or grid computing, the algorithm can reduce latency even more when InterruptThrottleRate is set to mode 1. In this mode, the InterruptThrottleRate will be increased stepwise to 70000 for traffic in class "Lowest latency". Setting InterruptThrottleRate to 0 turns off any interrupt moderation and may improve small packet latency, but is generally not suitable for bulk throughput traffic NOTE: Dynamic interrupt throttling is only applicable to adapters operating in MSI or Legacy interrupt mode, using a single receive queue. NOTE: When ixgbevf is loaded with default settings and multiple adapters are in use simultaneously, the CPU utilization may increase non-linearly. In order to limit the CPU utilization without impacting the overall throughput, we recommend that you load the driver as follows: modprobe ixgbevf InterruptThrottleRate=3000,3000,3000 This sets the InterruptThrottleRate to 3000 interrupts/sec for the first, second, and third instances of the driver. The range of 2000 to 3000 interrupts per second works on a majority of systems and is a good starting point, but the optimal value will be platform-specific. If CPU utilization is not a concern, use default driver settings.

## Additional Configurations

### Configuring the Driver on Different Distributions

Configuring a network driver to load properly when the system is started is distribution dependent. Typically, the configuration process involves adding an alias line to /etc/modules.conf or /etc/modprobe.conf as well as editing other system startup scripts and/or configuration files. Many popular Linux distributions ship with tools to make these changes for you. To learn the proper way to configure a network device for your system, refer to your distribution documentation. If during this process you are asked for the driver or module name, the name for the Linux Base Driver for the Gigabit Family of Adapters is ixgbevf.
As an example, if you install the ixgbevf driver for two Gigabit adapters (eth0 and eth1) and want to set the interrupt mode to MSI-X and MSI respectively, add the following to modules.conf or /etc/modprobe.conf:

> alias eth0 ixgbevf
> alias eth1 ixgbevf
> options ixgbevf InterruptThrottleRate=3,1

### Viewing Link Messages

Link messages will not be displayed to the console if the distribution is restricting system messages. In order to see network driver link messages on your console, set dmesg to eight by entering the following:

> dmesg -n 8

| NOTE: This setting is not saved across reboots.

### ethtool

The driver utilizes the ethtool interface for driver configuration and diagnostics, as well as displaying statistical information. ethtool version 3.0 or later is required for this functionality, although we strongly recommend downloading the latest version at:
http://ftp.kernel.org/pub/software/network/ethtool/

MACVLAN

ixgbevf supports MACVLAN on those kernels that have the feature included. Kernel support for MACVLAN can be tested by checking if the MACVLAN driver is loaded. The user can run 'lsmod | grep macvlan' to see if the MACVLAN driver is loaded or run 'modprobe macvlan' to try to load the MACVLAN driver.

It may be necessary to update to a recent release of the iproute2 package to get support of MACVLAN via the 'ip' command.

## Known Issues/Troubleshooting

| NOTE: After installing the driver, if your Intel Network Connection is not working, verify that you have installed the correct driver.

### Driver Compilation

When trying to compile the driver by running make install, the following error may occur:
"Linux kernel source not configured - missing version.h"
To solve this issue, create the version.h file by going to the Linux source tree and entering:

> make include/linux/version.h.

### Multiple Interfaces on Same Ethernet Broadcast Network

Due to the default ARP behavior on Linux, it is not possible to have one system on two IP networks in the same Ethernet broadcast domain (non-partitioned switch) behave as expected. All Ethernet interfaces will respond to IP traffic for any IP address assigned to the system. This results in unbalanced receive traffic.
If you have multiple interfaces in a server, either turn on ARP filtering by entering:

> echo 1 > /proc/sys/net/ipv4/conf/all/arp_filter

(this only works if your kernel's version is higher than 2.4.5)

| NOTE: This setting is not saved across reboots. The configuration change can be made permanent by adding the line: net.ipv4.conf.all.arp_filter = 1 to the file /etc/sysctl.conf or, install the interfaces in separate broadcast domains (either in different switches or in a switch partitioned to VLANs).

### Build error with Asianux 3.0 - redefinition of typedef 'irq_handler_t'

Some systems may experience build issues due to redefinition of irq_handler_t. To resolve this issue build the driver (step 4 above) using the command:

> make CFLAGS_EXTRA=-DAX_RELEASE_CODE=1 install

### MSI-X Issues with Kernels between 2.6.19 - 2.6.21 (inclusive)

Kernel panics and instability may be observed on any MSI-X hardware if you use irqbalance with kernels between 2.6.19 and 2.6.21. If such problems are encountered, you may disable the irqbalance daemon or upgrade to a newer kernel.

### Rx Page Allocation Errors

Page allocation failure. order:0 errors may occur under stress with kernels 2.6.25 and above. This is caused by the way the Linux kernel reports this stressed condition.

## Support

For general information, go to the Intel support website at:

www.intel.com/support/

If an issue is identified with the released source code on the supported kernel with a supported adapter, email the specific information related to the issue to linux.nics@intel.com.

`Last modified on 4/18/11 11:13a 10/22/04 9:45a 193`