# Installation and Configuration

This section provides how to install and setup Intel® Ethernet FCoE components.

Follow the detailed instructions in Microsoft* Windows Installation or Linux Installation.

## Enabling Intel® Ethernet FCoE Boot

In order to enable Intel® Ethernet FCoE Boot, the firmware should be loaded as Option ROM by the BIOS when the system boots. `"Intel(R) FCoE Boot"` followed by the firmware version number is displayed, if the firmware is installed correctly.

See instructions on Intel® Ethernet FCoE Boot.

`Last modified on 4/20/11 10:06a Revision 6`