# Switch Configuration for Intel® Ethernet FCoE Protocol Driver

Nexus/Cisco Switch Platform

Brocade Switch Platform

| NOTES: In the following examples, the assumption is made that the VLAN and VSAN configurations have already been performed. For more installation details check with your switch vendor's documentation: Cisco Nexus Brocade

## Cisco Nexus 5000 Series Switch Platform

For the Nexus/Cisco switch platform, a virtual interface is needed to bind the Ethernet port to the FC forwarder or FCF. Assume port 1/3 in the following example.

Commands to enable trunk mode for a Ether port

Configure

Interface Ethernet 1/3

switchport mode trunk

spanning-tree port type edge trunk

exit

Commands to create a VFC:

configure

interface vfc 3

bind interface Ethernet 1/3

no shutdown

exit

## Brocade 8000 Series FCoE Switch

For the Brocade 8000 series FCoE switch, assuming port 1/3, vlan 101 for FCoE, use:

configure terminal

interface TenGigabitEthernet 1/3

switchport

switchport mode converged

vlan classifier activate group 1 vlan 101

no shutdown

cee default

exit

Note: | The "cmsh" command must be issued before the "configure terminal" command will function properly.

`Last modified on 4/19/11 11:33a Revision 14`