  +------------------------------------------------------------------------+
  |    This report is created by ASTRA32 v.2.11  .  Nov-21-2011 20:38:35   |
  +------------------------------------------------------------------------+
                               A2KKV_XP

     Registered To:            Sysinfo Lab
     License Type:             Professional for 1 computer

                  +-----------------------------------------+
                  |              System Summary             |
                  +-----------------------------------------+
  Processor
     Processor:                AMD Phenom II X3 710
     CPU Clock:                2611.9 MHz (13.0 x 200.9 MHz)
     Level 1 Cache:            3 x 64+64 kB (data+instr.)
     Level 2 Cache:            3 x 512 kB
     Level 3 Cache:            1 x 6144 kB
  Motherboard
     System Name:              Gigabyte Technology Co., Ltd. GA-MA770T-UD3P
     Motherboard Vendor:       Gigabyte Technology Co., Ltd.
     Board Model:              Gigabyte Technology Co., Ltd. GA-MA770T-UD3P
     BIOS Version:             Award Modular BIOS v6.00PG
     Chipset Name:             AMD 770/780FX/790FX
     Chipset Vendor:           ATI Technologies Inc
     Chipset:                  RX790 GFX Single Slot
     Southbridge Vendor:       ATI Technologies Inc
     Southbridge:              SB700 LPC host controller
     DMI/SMBIOS Version:       2.4
  Memory
     Memory Size:              2094572 kB (2045.48 MB)
     System Memory:            2046 MB
     Memory Module:            1024MB DDR3-1333 (PC3-10600) SDRAM (Kingston)
     Memory Module:            1024MB DDR3-1333 (PC3-10600) SDRAM (Kingston)
  Storage
     Floppy Drive:             Floppy 1.44 MB (3.5")
     HDD Model:                WDC WD1001FALS-00J7B0
     HDD Size:                 953869 MB (931.51 GB)
     HDD Model:                Kingston DataTraveler II+
     HDD Size:                 491 MB (0.48 GB)
     CD/DVD Model:             _NEC DVD_RW ND-3550A
     CD/DVD Speed:             48x (Write: 48x)
     CD/DVD Model:             CD-W540E
     CD/DVD Speed:             48x (Write: 40x)
  Video
     Monitor Vendor:           LG Electronics Inc.
     Monitor Model:            LG FLATRON F920P
     Video Chip Vendor:        ATI Technologies Inc
     Video Chip:               RV770 [Radeon HD 4870]
     Video Memory Size:        512 MB
  Sound
     Sound Chip Vendor:        ATI Technologies Inc
     Sound Chip:               IXP SB600 High Definition Audio Controller
     AC'97/HDA Codec Name:     Realtek ALC888/ALC1200
     Sound Chip Vendor:        ATI Technologies Inc
     Sound Chip:               HD48x0 audio
     AC'97/HDA Codec Name:     ATI R600 HDMI
     Sound Chip Vendor:        Creative Labs
     Sound Chip:               EMU10K2 Audio Chipset (SB Audigy Series)
  Operating System
     Operating System:         MS Windows XP Professional (5.1.2600 Service Pack 2)
     Windows Folder:           H:\WINDOWS
  Network
     Network Name:             A2KKV_XP
     Interface Description:    TAP-Win32 Adapter V8 - Packet Scheduler Miniport
     MAC Address:              00-FF-0C-27-A1-46
     Adapter Vendor:           Realtek Semiconductor
     Adapter Name:             RTL8168/8111 PCI-E Gigabit Ethernet NIC
     Interface Description:    Realtek RTL8168C(P)/8111C(P) PCI-E Gigabit Ethernet NIC - Packet Scheduler Miniport
     MAC Address:              00-24-1D-89-15-40
  Ports
     LPT Ports:                None
     COM Ports:                COM1(03F8h)

                  +-----------------------------------------+
                  |               Motherboard               |
                  +-----------------------------------------+
  System
     System Vendor:            Gigabyte Technology Co., Ltd.
     Product Name:             GA-MA770T-UD3P
     Version:
     Serial Number:
     UUID:                     303032343144383931353430FFFFFFFF
     Wake-up Type:             Power Switch
     SKU Number:
     Family:
  Motherboard
     Motherboard Vendor:       Gigabyte Technology Co., Ltd.
     Vendor URL:               www.gigabyte.com.tw
     Board Model:              Gigabyte Technology Co., Ltd. GA-MA770T-UD3P
     Version:
     Serial Number:
     BIOS Version:             Award Modular BIOS v6.00PG
     BIOS Date:                03/11/11
     Chipset Name:             AMD 770/780FX/790FX
     Chipset Vendor:           ATI Technologies Inc
     Chipset:                  RX790 GFX Single Slot
     Southbridge Vendor:       ATI Technologies Inc
     Southbridge:              SB700 LPC host controller
  System Enclosure
     Manufacturer:             Gigabyte Technology Co., Ltd.
     Type:                     Desktop
     Version:
     Serial Number:
     Asset Tag:
     Boot-up State:            Unknown
     Power Supply State:       Unknown
     Thermal State:            Unknown
     Security Status:          Unknown
     OEM-defined:              00000000h

                  +-----------------------------------------+
                  |                  CPU                    |
                  +-----------------------------------------+
  CPU
     Processor:                AMD Phenom II X3 710
     Coprocessor:              Internal
     CPU Clock:                2611.9 MHz
     Level 1 Cache:            3 x 64+64 kB (data+instr.)
     Level 2 Cache:            3 x 512 kB
     Level 3 Cache:            1 x 6144 kB
     FSB Clock:                200.9 MHz
     Multiplier:               13.0
     Platform ID:              Socket AM2+/AM3
     Vendor:                   AuthenticAMD
     Processor Name:           AMD Phenom(tm) II X3 710 Processor
     Processor Type:           Original OEM Processor
     CPUID:                    Family: 15, Model: 4, Stepping: 2
     Ext. Family/Model:        Family: 1, Model: 0
     CPU Signature:            00100F42h
     Brand ID:                 Phenom II X3 710 (40A6h)
     Number of Cores:          3
     Logical CPU Count:        HTT Not Supported
     Max CPUID Level:          5
     Max ExtCPUID Level:       8000001Bh
     Code Name:                Heka (0.045mk)
     Core Stepping:            RB-C2
     MSR C0010064h:            800001FDh:3800240Ah
     MSR C0010065h:            800001EBh:38003403h
     MSR C0010066h:            800001DEh:3800444Ch
     MSR C0010067h:            80000187h:38005040h
     MSR C0010071h:            30B40093h:3800240Ah
  Instruction Set
     Floating-Point Unit On-Chip:         [X]
     IA MMX Technology:                   [X]
     SSE Instruction Set:                 [X]
     SSE2 Instruction Set:                [X]
     SSE3 Instruction Set:                [X]
     Supplemental SSE3 Instruction Set:   [ ]
     SSE4.1 Instruction Set:              [ ]
     SSE4.2 Instruction Set:              [ ]
     Advanced Vector Extensions (AVX):    [ ]
     FMA Instructions Set:                [ ]
     AES Instructions Set:                [ ]
     Intel Extended Memory 64 Tech.:      [ ]
     Intel Architecture - 64 (IA-64):     [ ]
     AMD MMX Instruction Extensions:      [X]
     AMD 3DNow! Instructions:             [X]
     AMD 3DNow! Extensions:               [X]
     AMD 3DNow! Prefetch:                 [X]
     AMD SSE4A Extensions:                [X]
     AMD eXtended OPeration (XOP):        [ ]
     AMD Misaligned SSE:                  [X]
     AMD64 Architecture:                  [X]
     Cyrix Extended MMX:                  [ ]
     CMPXCHG8 Instruction Supported:      [X]
     CMPXCHG16 Instruction Supported:     [X]
     Fast System Call:                    [X]
     Conditional Move Instruction:        [X]
     CLFLUSH Insruction Supported:        [X]
     Fast Save and Restore:               [X]
     Monitor/MWAIT Instructions:          [X]
     SYSCALL/SYSRET Instructions:         [X]
     LAHF/SAHF Instructions:              [X]
     POPCNT Insruction Supported:         [X]
     XSAVE Insructions Supported:         [ ]
     OS Supports XSAVE Instructions:      [ ]
     PCLMULQDQ Instruction Supported:     [ ]
     MOVBE Insruction Supported:          [ ]
     F16C Insruction Supported:           [ ]
     RDTSCP Insruction Supported:         [X]
     RDRAND Insruction Supported:         [ ]
     AMD Fast Save and Restore:           [X]
     AMD SKINIT, STGI, DEV Supported:     [X]
     AMD Light Weight Profiling (LWP):    [ ]
     AMD FMA4 Insruction Supported:       [ ]
     AMD TBM Insruction Supported:        [ ]
  Processor Features
     Virtual Mode Extension:              [X]
     Debugging Extension:                 [X]
     Page Size Extension:                 [X]
     Time Stamp Counter:                  [X]
     Model Specific Registers:            [X]
     Physical Address Extension:          [X]
     Machine Check Exception:             [X]
     On-chip APIC Hardware Supported:     [X]
     Memory Type Range Registers:         [X]
     Page Global Enable:                  [X]
     Machine Check Architecture:          [X]
     Page Attribute Table:                [X]
     36-bit Page Size Extension:          [X]
     Processor Serial Number:             [ ]
     Debug Store:                         [ ]
     64-bit Debug Store:                  [ ]
     Self-Snoop:                          [ ]
     Hyper-Threading Technology:          [ ]
     Pending Break Enable:                [ ]
     CPL-Qualified Debug Store:           [ ]
     L1 Context ID:                       [ ]
     Send Task Priority Messages:         [ ]
     Direct Cache Access:                 [ ]
     Performance Capabilities MSR:        [ ]
     x2APIC Architecture:                 [ ]
     Advanced Bit Manipulation:           [X]
     OS Visible Workaround:               [X]
     Instruction Based Sampling:          [X]
     1-GB Large Page:                     [X]
     Process Context Identifiers:         [ ]
     Time Stamp Counter Deadline:         [ ]
     Intel Virtualization Technology:     [ ]
     Intel Trusted Execution Technology:  [ ]
     AMD Core Performance Boost:          [ ]
     AMD No-execute Page Protection:      [X]
     AMD Secure Virtual Machine:          [X]
     AMD Model-Specific Registers:        [X]
     AMD Multiprocessing Capable:         [ ]
     AMD CMP Legacy Mode:                 [X]
     AMD CR8 in Legacy Mode:              [X]
     AMD Ext. APIC Register Space:        [X]
     AMD Watchdog Timer:                  [X]
     AMD Translation Cache Extension:     [ ]
     AMD Topology Extensions:             [ ]
     AMD Core Performance Counter Ext.:   [ ]
     AMD NB Performance Counter Ext.:     [ ]
  Power Management
     ACPI Supported:                      [ ]
     Thermal Monitor Supported:           [ ]
     Thermal Monitor 2:                   [ ]
     Enhanced SpeedStep Technology:       [ ]
     Digital Thermal Sensor:              [ ]
     Operating Point Protection:          [ ]
     Invariant TSC:                       [X]
     AMD Temperature Sensor:              [X]
     AMD Frequency ID Control:            [ ]
     AMD Voltage ID Control:              [ ]
     AMD Thermal Trip:                    [X]
     AMD Thermal Monitoring:              [X]
     AMD Software Thermal Control:        [X]
     AMD 100MHz Multiplier Steps:         [X]
     AMD Hardware P-State Control:        [X]

                  +-----------------------------------------+
                  |                CPU Cache                |
                  +-----------------------------------------+
  Level 1 Instruction Cache
     Size:                     3 x 64 kB
     Associativity:            2-way
     Lines per Tag:            1
     Line Size:                64 byte
     TLB 4K Pages:
       Number of Entries:      32
       Associativity:          full
     TLB 2/4M Pages:
       Number of Entries:      16
       Associativity:          full
  Level 1 Data Cache
     Size:                     3 x 64 kB
     Associativity:            2-way
     Lines per Tag:            1
     Line Size:                64 byte
     TLB 4K Pages:
       Number of Entries:      48
       Associativity:          full
     TLB 2/4M Pages:
       Number of Entries:      48
       Associativity:          full
  Level 2 Cache
     Size:                     3 x 512 kB
     Associativity:            16-way
     Lines per Tag:            1
     Line Size:                64 byte
     Instr. TLB 4K Pages:
       Number of Entries:      512
       Associativity:          4-way
     Data TLB 4K Pages:
       Number of Entries:      512
       Associativity:          4-way
     Instr. TLB 2/4M Pages:
       Number of Entries:      0
       Associativity:          off
     Data TLB 2/4M Pages:
       Number of Entries:      128
       Associativity:          2-way
  Level 3 Cache
     Size:                     1 x 6144 kB
     Associativity:            48-way
     Line Size:                64 byte

                  +-----------------------------------------+
                  |              CPU (SMBIOS)               |
                  +-----------------------------------------+
  Processor
     Processor Vendor:         AMD
     Processor Version:        AMD Phenom(tm) II X3 710 Processor
     Current Speed:            2600 MHz
     External Clock:           200 MHz
     Voltage:                  1.3 V
     Processor Upgrade:        ZIF Socket
     Processor Status:         CPU Enabled
     Socket Designation:       Socket M2
     Processor Type:           Central Processor
     Processor Family:         AMD Athlon
     Processor ID1:            00100F42h
     Processor ID2:            178BFBFFh
     Max Speed:                3200 MHz
     Socket Status:            CPU Socket Populated
     Serial Number:
     Asset Tag:
     Part Number:
     Structure Length:         23h

                  +-----------------------------------------+
                  |            CPU (SMBIOS) Cache           |
                  +-----------------------------------------+
  Level 1 Cache
     Installed Size:           128 kB
     Operational Mode:         Write Back
     Current SRAM Type:        Synchronous
     Status:                   Enabled
     Socket Designation:       Internal Cache
     Cache Socketed:           Not Socketed
     Location:                 Internal
     Maximum Cache Size:       128 kB
     Supported SRAM Type:      Synchronous
     Cache Speed:              Unknown
     Error Correction:         Unknown
     System Cache Type:        Unknown
     Associativity:            Unknown
     Structure Length:         13h
  Level 1 Cache
     Installed Size:           128 kB
     Operational Mode:         Write Back
     Current SRAM Type:        Synchronous
     Status:                   Enabled
     Socket Designation:       Internal Cache
     Cache Socketed:           Not Socketed
     Location:                 Internal
     Maximum Cache Size:       128 kB
     Supported SRAM Type:      Synchronous
     Cache Speed:              Unknown
     Error Correction:         Unknown
     System Cache Type:        Unknown
     Associativity:            Unknown
     Structure Length:         13h
  Level 3 Cache
     Installed Size:           512 kB
     Operational Mode:         Write Back
     Current SRAM Type:        Synchronous
     Status:                   Enabled
     Socket Designation:       External Cache
     Cache Socketed:           Not Socketed
     Location:                 Internal
     Maximum Cache Size:       512 kB
     Supported SRAM Type:      Synchronous
     Cache Speed:              Unknown
     Error Correction:         Unknown
     System Cache Type:        Unknown
     Associativity:            Unknown
     Structure Length:         13h
  Level 2 Cache
     Installed Size:           0 kB
     Operational Mode:         Write Through
     Current SRAM Type:        Synchronous
     Status:                   Disabled
     Socket Designation:       External Cache
     Cache Socketed:           Not Socketed
     Location:                 Internal
     Maximum Cache Size:       1024 kB
     Supported SRAM Type:      Synchronous
     Cache Speed:              Unknown
     Error Correction:         Unknown
     System Cache Type:        Unknown
     Associativity:            Unknown
     Structure Length:         13h

                  +-----------------------------------------+
                  |                  BIOS                   |
                  +-----------------------------------------+
  BIOS
     Motherboard Vendor:       Gigabyte Technology Co., Ltd.
     Vendor URL:               www.gigabyte.com.tw
     BIOS Version:             Award Modular BIOS v6.00PG
     BIOS Date:                03/11/11
     BIOS Copyright:           Award Software Inc. - 04/23/90
     Motherboard ID:           AMD 770 BIOS for GA-MA770T-UD3P F11
     BIOS ID:                  03/11/2011-RX780-SB710-7A66AG05C-00
     BIOS Type:                Phoenix Award BIOS v6.00
     Bus Type:                 ISA/PCI
     Processor:                686
     Chipset:                  AMD 790FX
     Chipset ID:               RX780-SB710
     BIOS Revision:            00
     MP Specification Ver.:    1.4
     MP Table Address:         000Fh:1100h
     Number of CPU/Cores:      3
     DMI/SMBIOS Version:       2.4
     DMI/SMBIOS Structures:    55
     DMI/SMBIOS Address:       000Fh:0100h
  SMBIOS
     BIOS Vendor:              Award Software International, Inc.
     BIOS Version:             F11
     BIOS Date:                03/11/2011
     BIOS ROM Size:            1024 kB
     Starting Segment:         E000h
     Current Language:         n|US|iso8859-1
     Number of Languages:      3
     Structure Length:         18h
  Bus Supported
     PCI is Supported:                    [X]
     AGP is Supported:                    [ ]
     USB is Supported:                    [X]
     ISA is Supported:                    [X]
     VLBus is Supported:                  [ ]
     MCA is Supported:                    [ ]
     EISA is Supported:                   [ ]
     PC Card is Supported:                [ ]
  Boot Options
     Selectable Boot:                     [X]
     Boot From CD:                        [X]
     ATAPI ZIP Drive Boot:                [X]
     LS-120 Boot:                         [X]
     BIOS Boot Specification:             [X]
     Boot From PC Card:                   [ ]
     Network Service Boot Supported:      [ ]
     I2O Boot:                            [ ]
     1394 Boot:                           [ ]
  BIOS Features
     BIOS Characteristics:                [X]
     ACPI Supported:                      [X]
     PnP is Supported:                    [X]
     APM is Supported:                    [X]
     ESCD Support:                        [ ]
     Enhanced Disk Drive (EDD):           [X]
     BIOS is Upgradeable (Flash):         [X]
     BIOS ROM is Socketed:                [X]
     BIOS Shadowing is Allowed:           [X]
     Smart Battery Supported:             [ ]
     Targeted Content Distribution:       [X]
     UEFI Specification is Supported:     [ ]
     Virtual Machine:                     [ ]
     Int 13h - 5.25"/360kB Floppy:        [X]
     Int 13h - 5.25"/1.2MB Floppy:        [X]
     Int 13h - 3.5"/720kB Floppy:         [X]
     Int 13h - 3.5"/2.88MB Floppy:        [X]
     Int 5h, Print Screen Service:        [X]
     Int 9h, 8042 Keyboard Services:      [X]
     Int 14h, Serial Services:            [X]
     Int 17h, Printer Services:           [X]
     Int 10h, CGA/Mono Video Services:    [X]
     Int 13h - Floppy for NEC 9800:       [ ]
     Int 13h - Floppy for Toshiba:        [ ]
     NEC PC-98:                           [ ]
  Other SMBIOS Structures
     Memory Array Mapped Address (19)
     Memory Device Mapped Address (20)
     Memory Device Mapped Address (20)
     Memory Device Mapped Address (20)
     Memory Device Mapped Address (20)
     System Boot Information (32)
     Unknown (188)
     Unknown (190)
     Unknown (192)
     Unknown (194)
     Unknown (196)
     Unknown (198)

                  +-----------------------------------------+
                  |             PCI/AGP Devices             |
                  +-----------------------------------------+
  Bus: 00h, Device: 00h, Function: 00h
     Vendor (1002h):           ATI Technologies Inc
     Device (5957h):           RX790 GFX Single Slot
     Subsys Vendor (1002h):    ATI Technologies Inc
     Subsystem ID (5957h):     Unknown
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           E0000000h - FFFFFFFFh
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       PCI standard host CPU bridge
     Device Class:             System
     Device Location:          PCI bus 0, device 0, function 0
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 machine.inf
     Hardware ID:              PCI\VEN_1002&DEV_5957&SUBSYS_00000000&REV_00
     Compatible ID:            PCI\VEN_1002&CC_060000

  Bus: 00h, Device: 02h, Function: 00h
     Vendor (1002h):           ATI Technologies Inc
     Device (5978h):           RD790 PCI to PCI bridge (external gfx0 port A)
     Class (06h):              Bridge
     SubClass (04h):           PCI/PCI
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Base I/O Port:            E000h - EFFFh
     Memory Address:           FDF00000h - FDFFFFFFh
     Memory Address:           D0000000h - DFFFFFFFh
     System IRQ:               18
     Interrupt Pin:            INTA#
  PCI-E Capabilities
     PCI Express Version:      2
     Link Speed:               5.0 GB/s (Current: 5.0 GB/s)
     Link Width:               x16 (Current: x16)
     Link Port Number:         0
     Physical Slot Number:     0
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       PCI standard PCI-to-PCI bridge
     Device Class:             System
     Device Location:          PCI bus 0, device 2, function 0
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 machine.inf
     Service Name:             pci
     Hardware ID:              PCI\VEN_1002&DEV_5978&SUBSYS_00000000&REV_00
     Compatible ID:            PCI\VEN_1002&CC_060400

  Bus: 00h, Device: 0Ah, Function: 00h
     Vendor (1002h):           ATI Technologies Inc
     Device (597Fh):           RD790 PCI to PCI bridge (PCIe gpp port F)
     Class (06h):              Bridge
     SubClass (04h):           PCI/PCI
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Base I/O Port:            D000h - DFFFh
     Memory Address:           FDE00000h - FDEFFFFFh
     Memory Address:           FDB00000h - FDBFFFFFh
     System IRQ:               18
     Interrupt Pin:            INTA#
  PCI-E Capabilities
     PCI Express Version:      2
     Link Speed:               5.0 GB/s (Current: 2.5 GB/s)
     Link Width:               x1 (Current: x1)
     Link Port Number:         5
     Physical Slot Number:     1
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       PCI standard PCI-to-PCI bridge
     Device Class:             System
     Device Location:          PCI bus 0, device 10, function 0
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 machine.inf
     Service Name:             pci
     Hardware ID:              PCI\VEN_1002&DEV_597F&SUBSYS_00000000&REV_00
     Compatible ID:            PCI\VEN_1002&CC_060400

  Bus: 00h, Device: 11h, Function: 00h
     Vendor (1002h):           ATI Technologies Inc
     Device (4390h):           SB700 SATA Controller [IDE mode]
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (B002h):     GA-MA770-DS3rev2.0 Motherboard
     Class (01h):              Storage
     SubClass (01h):           IDE
     Revision:                 00h
     Interface:                8Fh
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Base I/O Port:            0000FF00h - 0000FF07h
     Base I/O Port:            0000FE00h - 0000FE03h
     Base I/O Port:            0000FD00h - 0000FD07h
     Base I/O Port:            0000FC00h - 0000FC03h
     Base I/O Port:            0000FB00h - 0000FB0Fh
     Memory Address:           FE02F000h - FE02F3FFh
     System IRQ:               22
     Interrupt Pin:            INTA#
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard IDE ATA/ATAPI controllers)
     Device Description:       Standard Dual Channel PCI IDE Controller
     Device Class:             hdc
     Device Location:          PCI bus 0, device 17, function 0
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 mshdc.inf
     Service Name:             pciide
     Hardware ID:              PCI\VEN_1002&DEV_4390&SUBSYS_B0021458&REV_00
     Compatible ID:            PCI\VEN_1002&DEV_4390&REV_00

  Bus: 00h, Device: 12h, Function: 00h
     Vendor (1002h):           ATI Technologies Inc
     Device (4397h):           SB700 USB OHCI0 Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5004h):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 00h
     Interface:                10h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           FE02E000h - FE02EFFFh
     System IRQ:               16
     Interrupt Pin:            INTA#
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard USB Host Controller)
     Device Description:       Standard OpenHCD USB Host Controller
     Device Class:             USB
     Device Location:          PCI bus 0, device 18, function 0
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 usbport.inf
     Service Name:             usbohci
     Hardware ID:              PCI\VEN_1002&DEV_4397&SUBSYS_50041458&REV_00
     Compatible ID:            PCI\VEN_1002&DEV_4397&REV_00

  Bus: 00h, Device: 12h, Function: 01h
     Vendor (1002h):           ATI Technologies Inc
     Device (4398h):           SB700 USB OHCI1 Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5004h):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 00h
     Interface:                10h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           FE02D000h - FE02DFFFh
     System IRQ:               16
     Interrupt Pin:            INTA#
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard USB Host Controller)
     Device Description:       Standard OpenHCD USB Host Controller
     Device Class:             USB
     Device Location:          PCI bus 0, device 18, function 1
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 usbport.inf
     Service Name:             usbohci
     Hardware ID:              PCI\VEN_1002&DEV_4398&SUBSYS_50041458&REV_00
     Compatible ID:            PCI\VEN_1002&DEV_4398&REV_00

  Bus: 00h, Device: 12h, Function: 02h
     Vendor (1002h):           ATI Technologies Inc
     Device (4396h):           SB700 USB EHCI Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5004h):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 00h
     Interface:                20h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           FE02C000h - FE02C0FFh
     System IRQ:               17
     Interrupt Pin:            INTB#
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard USB Host Controller)
     Device Description:       Standard Enhanced PCI to USB Host Controller
     Device Class:             USB
     Device Location:          PCI bus 0, device 18, function 2
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.0
     Driver Date:              6-1-2002
     Inf File:                 usbport.inf
     Service Name:             usbehci
     Hardware ID:              PCI\VEN_1002&DEV_4396&SUBSYS_50041458&REV_00
     Compatible ID:            PCI\VEN_1002&DEV_4396&REV_00

  Bus: 00h, Device: 13h, Function: 00h
     Vendor (1002h):           ATI Technologies Inc
     Device (4397h):           SB700 USB OHCI0 Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5004h):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 00h
     Interface:                10h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           FE02B000h - FE02BFFFh
     System IRQ:               18
     Interrupt Pin:            INTA#
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard USB Host Controller)
     Device Description:       Standard OpenHCD USB Host Controller
     Device Class:             USB
     Device Location:          PCI bus 0, device 19, function 0
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 usbport.inf
     Service Name:             usbohci
     Hardware ID:              PCI\VEN_1002&DEV_4397&SUBSYS_50041458&REV_00
     Compatible ID:            PCI\VEN_1002&DEV_4397&REV_00

  Bus: 00h, Device: 13h, Function: 01h
     Vendor (1002h):           ATI Technologies Inc
     Device (4398h):           SB700 USB OHCI1 Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5004h):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 00h
     Interface:                10h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           FE02A000h - FE02AFFFh
     System IRQ:               18
     Interrupt Pin:            INTA#
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard USB Host Controller)
     Device Description:       Standard OpenHCD USB Host Controller
     Device Class:             USB
     Device Location:          PCI bus 0, device 19, function 1
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 usbport.inf
     Service Name:             usbohci
     Hardware ID:              PCI\VEN_1002&DEV_4398&SUBSYS_50041458&REV_00
     Compatible ID:            PCI\VEN_1002&DEV_4398&REV_00

  Bus: 00h, Device: 13h, Function: 02h
     Vendor (1002h):           ATI Technologies Inc
     Device (4396h):           SB700 USB EHCI Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5004h):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 00h
     Interface:                20h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           FE029000h - FE0290FFh
     System IRQ:               19
     Interrupt Pin:            INTB#
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard USB Host Controller)
     Device Description:       Standard Enhanced PCI to USB Host Controller
     Device Class:             USB
     Device Location:          PCI bus 0, device 19, function 2
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.0
     Driver Date:              6-1-2002
     Inf File:                 usbport.inf
     Service Name:             usbehci
     Hardware ID:              PCI\VEN_1002&DEV_4396&SUBSYS_50041458&REV_00
     Compatible ID:            PCI\VEN_1002&DEV_4396&REV_00

  Bus: 00h, Device: 14h, Function: 00h
     Vendor (1002h):           ATI Technologies Inc
     Device (4385h):           IXP SB600 SMBUS Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (4385h):     GA-MA770-DS3rev2.0 Motherboard
     Class (0Ch):              Serial
     SubClass (05h):           SMBus Controller
     Revision:                 3Ch
     Interface:                00h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [ ]
     66 MHz Speed Support:     [X]
  Device Resources
     SMBus Port:               0B00h
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             ATI Technologies Inc
     Device Description:       ATI SMBus
     Device Class:             System
     Device Location:          PCI bus 0, device 20, function 0
     Driver Provider:          ATI Technologies Inc
     Driver Version:           5.10.1000.8
     Driver Date:              2-26-2007
     Inf File:                 oem5.inf
     Hardware ID:              PCI\VEN_1002&DEV_4385&SUBSYS_43851458&REV_3C
     Compatible ID:            PCI\VEN_1002&DEV_4385&REV_3C

  Bus: 00h, Device: 14h, Function: 01h
     Vendor (1002h):           ATI Technologies Inc
     Device (439Ch):           SB700 IDE
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5002h):     Unknown
     Class (01h):              Storage
     SubClass (01h):           IDE
     Revision:                 00h
     Interface:                8Ah
  Device Properties
     Device Timing:            Medium
     Memory Access:            [ ]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Base I/O Port:            0000FA00h - 0000FA0Fh
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard IDE ATA/ATAPI controllers)
     Device Description:       Standard Dual Channel PCI IDE Controller
     Device Class:             hdc
     Device Location:          PCI bus 0, device 20, function 1
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 mshdc.inf
     Service Name:             pciide
     Hardware ID:              PCI\VEN_1002&DEV_439C&SUBSYS_50021458&REV_00
     Compatible ID:            PCI\VEN_1002&DEV_439C&REV_00

  Bus: 00h, Device: 14h, Function: 02h
     Vendor (1002h):           ATI Technologies Inc
     Device (4383h):           IXP SB600 High Definition Audio Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (A002h):     Unknown
     Class (04h):              Multimedia
     SubClass (03h):           Hi-definition Audio
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Slow
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Memory Address:           FE024000h - FE027FFFh
     System IRQ:               16
     Interrupt Pin:            INTA#
  AC'97/HDA Capabilities
     AC'97/HDA Codec Name:     Realtek ALC888/ALC1200
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             Microsoft
     Device Description:       Microsoft UAA Bus Driver for High Definition Audio
     Device Class:             System
     Device Location:          PCI bus 0, device 20, function 2
     Driver Provider:          Microsoft
     Driver Version:           5.10.0.5010
     Driver Date:              3-5-2004
     Inf File:                 hdaudbus.inf
     Service Name:             HDAudBus
     Hardware ID:              PCI\VEN_1002&DEV_4383&SUBSYS_A0021458&REV_00
     Compatible ID:            PCI\VEN_1002&DEV_4383&REV_00

  Bus: 00h, Device: 14h, Function: 03h
     Vendor (1002h):           ATI Technologies Inc
     Device (439Dh):           SB700 LPC host controller
     Subsys Vendor (1002h):    ATI Technologies Inc
     Subsystem ID (439Dh):     Unknown
     Class (06h):              Bridge
     SubClass (01h):           PCI/ISA
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       PCI standard ISA bridge
     Device Class:             System
     Device Location:          PCI bus 0, device 20, function 3
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 machine.inf
     Service Name:             isapnp
     Hardware ID:              PCI\VEN_1002&DEV_439D&SUBSYS_00000000&REV_00
     Compatible ID:            PCI\VEN_1002&CC_060100

  Bus: 00h, Device: 14h, Function: 04h
     Vendor (1002h):           ATI Technologies Inc
     Device (4384h):           IXP SB600 PCI to PCI Bridge
     Class (06h):              Bridge
     SubClass (04h):           PCI/PCI
     Revision:                 00h
     Interface:                01h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       PCI standard PCI-to-PCI bridge
     Device Class:             System
     Device Location:          PCI bus 0, device 20, function 4
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 machine.inf
     Service Name:             pci
     Hardware ID:              PCI\VEN_1002&DEV_4384&SUBSYS_00000000&REV_00
     Compatible ID:            PCI\VEN_1002&CC_060401

  Bus: 00h, Device: 14h, Function: 05h
     Vendor (1002h):           ATI Technologies Inc
     Device (4399h):           SB700 USB OHCI2 Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5004h):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 00h
     Interface:                10h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           FE028000h - FE028FFFh
     System IRQ:               18
     Interrupt Pin:            INTC#
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard USB Host Controller)
     Device Description:       Standard OpenHCD USB Host Controller
     Device Class:             USB
     Device Location:          PCI bus 0, device 20, function 5
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 usbport.inf
     Service Name:             usbohci
     Hardware ID:              PCI\VEN_1002&DEV_4399&SUBSYS_50041458&REV_00
     Compatible ID:            PCI\VEN_1002&DEV_4399&REV_00

  Bus: 00h, Device: 18h, Function: 00h
     Vendor (1022h):           Advanced Micro Devices (AMD)
     Device (1200h):           K10 [Opteron, Athlon64, Sempron] HyperTransport Configuration
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [ ]
     Bus Master:               [ ]
     66 MHz Speed Support:     [ ]
  Device Resources
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       PCI standard host CPU bridge
     Device Class:             System
     Device Location:          PCI bus 0, device 24, function 0
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 machine.inf
     Hardware ID:              PCI\VEN_1022&DEV_1200&SUBSYS_00000000&REV_00
     Compatible ID:            PCI\VEN_1022&CC_060000

  Bus: 00h, Device: 18h, Function: 01h
     Vendor (1022h):           Advanced Micro Devices (AMD)
     Device (1201h):           K10 [Opteron, Athlon64, Sempron] Address Map
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [ ]
     Bus Master:               [ ]
     66 MHz Speed Support:     [ ]
  Device Resources
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       PCI standard host CPU bridge
     Device Class:             System
     Device Location:          PCI bus 0, device 24, function 1
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 machine.inf
     Hardware ID:              PCI\VEN_1022&DEV_1201&SUBSYS_00000000&REV_00
     Compatible ID:            PCI\VEN_1022&CC_060000

  Bus: 00h, Device: 18h, Function: 02h
     Vendor (1022h):           Advanced Micro Devices (AMD)
     Device (1202h):           K10 [Opteron, Athlon64, Sempron] DRAM Controller
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [ ]
     Bus Master:               [ ]
     66 MHz Speed Support:     [ ]
  Device Resources
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       PCI standard host CPU bridge
     Device Class:             System
     Device Location:          PCI bus 0, device 24, function 2
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 machine.inf
     Hardware ID:              PCI\VEN_1022&DEV_1202&SUBSYS_00000000&REV_00
     Compatible ID:            PCI\VEN_1022&CC_060000

  Bus: 00h, Device: 18h, Function: 03h
     Vendor (1022h):           Advanced Micro Devices (AMD)
     Device (1203h):           K10 [Opteron, Athlon64, Sempron] Miscellaneous Control
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [ ]
     Bus Master:               [ ]
     66 MHz Speed Support:     [ ]
  Device Resources
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       PCI standard host CPU bridge
     Device Class:             System
     Device Location:          PCI bus 0, device 24, function 3
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 machine.inf
     Hardware ID:              PCI\VEN_1022&DEV_1203&SUBSYS_00000000&REV_00
     Compatible ID:            PCI\VEN_1022&CC_060000

  Bus: 00h, Device: 18h, Function: 04h
     Vendor (1022h):           Advanced Micro Devices (AMD)
     Device (1204h):           K10 [Opteron, Athlon64, Sempron] Link Control
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [ ]
     Bus Master:               [ ]
     66 MHz Speed Support:     [ ]
  Device Resources
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       PCI standard host CPU bridge
     Device Class:             System
     Device Location:          PCI bus 0, device 24, function 4
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 machine.inf
     Hardware ID:              PCI\VEN_1022&DEV_1204&SUBSYS_00000000&REV_00
     Compatible ID:            PCI\VEN_1022&CC_060000

  Bus: 01h, Device: 00h, Function: 00h
     Vendor (1002h):           ATI Technologies Inc
     Device (9440h):           RV770 [Radeon HD 4870]
     Subsys Vendor (1787h):    Hightech Information System Ltd (Medion??)
     Subsystem ID (2267h):     Unknown
     Class (03h):              Display
     SubClass (00h):           VGA
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Memory Address:           D0000000h - DFFFFFFFh
     Memory Address:           FDFE0000h - FDFEFFFFh
     Base I/O Port:            0000EE00h - 0000EEFFh
     System IRQ:               18
     Interrupt Pin:            INTA#
  PCI-E Capabilities
     PCI Express Version:      2
     Link Speed:               5.0 GB/s (Current: 5.0 GB/s)
     Link Width:               x16 (Current: x16)
     Link Port Number:         0
     Physical Slot Number:     0
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             ATI Technologies Inc.
     Device Description:       ATI Radeon HD 4800 Series
     Device Class:             Display
     Device Location:          PCI bus 1, device 0, function 0
     Driver Provider:          ATI Technologies Inc.
     Driver Version:           8.753.0.0
     Driver Date:              7-6-2010
     Inf File:                 oem7.inf
     Service Name:             ati2mtag
     Hardware ID:              PCI\VEN_1002&DEV_9440&SUBSYS_22671787&REV_00
     Compatible ID:            PCI\VEN_1002&DEV_9440&REV_00

  Bus: 01h, Device: 00h, Function: 01h
     Vendor (1002h):           ATI Technologies Inc
     Device (AA30h):           HD48x0 audio
     Subsys Vendor (1787h):    Hightech Information System Ltd (Medion??)
     Subsystem ID (AA30h):     Unknown
     Class (04h):              Multimedia
     SubClass (03h):           Hi-definition Audio
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Memory Address:           FDFFC000h - FDFFFFFFh
     System IRQ:               19
     Interrupt Pin:            INTB#
  AC'97/HDA Capabilities
     AC'97/HDA Codec Name:     ATI R600 HDMI
  PCI-E Capabilities
     PCI Express Version:      2
     Link Speed:               5.0 GB/s (Current: 5.0 GB/s)
     Link Width:               x16 (Current: x16)
     Link Port Number:         0
     Physical Slot Number:     0
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             Microsoft
     Device Description:       Microsoft UAA Bus Driver for High Definition Audio
     Device Class:             System
     Device Location:          PCI bus 1, device 0, function 1
     Driver Provider:          Microsoft
     Driver Version:           5.10.0.5010
     Driver Date:              3-5-2004
     Inf File:                 hdaudbus.inf
     Service Name:             HDAudBus
     Hardware ID:              PCI\VEN_1002&DEV_AA30&SUBSYS_AA301787&REV_00
     Compatible ID:            PCI\VEN_1002&DEV_AA30&REV_00

  Bus: 02h, Device: 00h, Function: 00h
     Vendor (10ECh):           Realtek Semiconductor
     Device (8168h):           RTL8168/8111 PCI-E Gigabit Ethernet NIC
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (E000h):     GA-EP45-DS5 Motherboard
     Class (02h):              Network
     SubClass (00h):           Ethernet
     Revision:                 02h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Base I/O Port:            0000DC00h - 0000DCFFh
     Memory Address:           FDBFF000h - FDBFFFFFh
     Memory Address:           FDBE0000h - FDBEFFFFh
     System IRQ:               18
     Interrupt Pin:            INTA#
  PCI-E Capabilities
     PCI Express Version:      1
     Link Speed:               2.5 GB/s (Current: 2.5 GB/s)
     Link Width:               x1 (Current: x1)
     Link Port Number:         0
     Physical Slot Number:     0
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             Realtek Semiconductor Corp.
     Device Description:       Realtek RTL8168C(P)/8111C(P) PCI-E Gigabit Ethernet NIC
     Device Class:             Net
     Device Location:          PCI bus 2, device 0, function 0
     Driver Provider:          Realtek Semiconductor Corp.
     Driver Version:           5.708.1030.2008
     Driver Date:              10-30-2008
     Inf File:                 oem4.inf
     Service Name:             RTLE8023xp
     Hardware ID:              PCI\VEN_10EC&DEV_8168&SUBSYS_E0001458&REV_02
     Compatible ID:            PCI\VEN_10EC&DEV_8168&REV_02

  Bus: 03h, Device: 06h, Function: 00h
     Vendor (1102h):           Creative Labs
     Device (0004h):           EMU10K2 Audio Chipset (SB Audigy Series)
     Subsys Vendor (1102h):    Creative Labs
     Subsystem ID (2005h):     Unknown
     Class (04h):              Multimedia
     SubClass (01h):           Audio
     Revision:                 04h
     Interface:                00h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [ ]
     I/O Access:               [ ]
     Bus Master:               [ ]
     66 MHz Speed Support:     [ ]
  Device Resources
     Base I/O Port:            0000CF00h - 0000CF3Fh
     System IRQ:               20
     Interrupt Pin:            INTA#
  Driver
     Driver Status:            The device is disabled (22)
     Manufacturer:             Creative Technology, Ltd.
     Device Description:       Creative Audigy Audio Processor (WDM)
     Friendly Name:            Creative SB Audigy 2 ZS (WDM)
     Device Class:             MEDIA
     Device Location:          PCI bus 3, device 6, function 0
     Driver Provider:          Creative
     Driver Version:           5.12.8.1164
     Driver Date:              12-8-2005
     Inf File:                 oem9.inf
     Service Name:             ctaud2k
     Hardware ID:              PCI\VEN_1102&DEV_0004&SUBSYS_20051102&REV_04
     Compatible ID:            PCI\VEN_1102&DEV_0004&REV_04

  Bus: 03h, Device: 0Eh, Function: 00h
     Vendor (104Ch):           Texas Instruments (TI)
     Device (8024h):           TSB43AB23 1394a-2000 OHCI PHY/link-layer Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (1000h):     GA-EP45-DS5 Motherboard
     Class (0Ch):              Serial
     SubClass (00h):           Firewire
     Revision:                 00h
     Interface:                10h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Memory Address:           FDDFF000h - FDDFF7FFh
     Memory Address:           FDDF8000h - FDDFBFFFh
     System IRQ:               22
     Interrupt Pin:            INTA#
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             Texas Instruments
     Device Description:       Texas Instruments OHCI Compliant IEEE 1394 Host Controller
     Device Class:             1394
     Device Location:          PCI bus 3, device 14, function 0
     Driver Provider:          Microsoft
     Driver Version:           5.1.2535.0
     Driver Date:              7-1-2001
     Inf File:                 1394.inf
     Service Name:             ohci1394
     Hardware ID:              PCI\VEN_104C&DEV_8024&SUBSYS_10001458&REV_00
     Compatible ID:            PCI\VEN_104C&DEV_8024&REV_00

                  +-----------------------------------------+
                  |              Memory Modules             |
                  +-----------------------------------------+
  Memory Slot 1
     Memory Type:              1024MB DDR3-1333 (PC3-10600) SDRAM
     Manufacturer:             Kingston
     Module Type:              Unbuffered DIMM
     Number of Ranks/Banks:    1 Ranks, 8 Banks
     Module Attributes:        Unbuffered
     Error Checking:           None
     CAS# Latency:             9.0 (Cycle Time: 1.500ns/686MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 9.0-9-9-24)
                               (tWR-tRC: 10-33)
     CAS# Latency:             8.0 (Cycle Time: 1.371ns/610MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 8.0-8-8-22)
                               (tWR-tRC: 10-30)
     CAS# Latency:             7.0 (Cycle Time: 1.200ns/533MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 7.0-7-7-20)
                               (tWR-tRC: 8-27)
     CAS# Latency:             6.0 (Cycle Time: 1.029ns/457MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 6.0-6-6-17)
                               (tWR-tRC: 7-23)
     Refresh Rate:             7.8 us (2X 85-95 C)
     Data Width:               64 bits
     SDRAM Width:              x8
     Voltage Interface:        1.5 V
     Max Case Temperature:     95 C (203 F)
     SPD Revision:             1.0
     Part Number:              9905402-015.A03LF
     Manufacturing Location:   China
     Manufacture Date:         September 2009 (0926h)
     Serial Number:            14CC41B4h
     Revision Code:            None
     EPP Support:              [ ]
     XMP Support:              [ ]

  Memory Slot 2
     Memory Type:              1024MB DDR3-1333 (PC3-10600) SDRAM
     Manufacturer:             Kingston
     Module Type:              Unbuffered DIMM
     Number of Ranks/Banks:    1 Ranks, 8 Banks
     Module Attributes:        Unbuffered
     Error Checking:           None
     CAS# Latency:             9.0 (Cycle Time: 1.500ns/686MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 9.0-9-9-24)
                               (tWR-tRC: 10-33)
     CAS# Latency:             8.0 (Cycle Time: 1.371ns/610MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 8.0-8-8-22)
                               (tWR-tRC: 10-30)
     CAS# Latency:             7.0 (Cycle Time: 1.200ns/533MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 7.0-7-7-20)
                               (tWR-tRC: 8-27)
     CAS# Latency:             6.0 (Cycle Time: 1.029ns/457MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 6.0-6-6-17)
                               (tWR-tRC: 7-23)
     Refresh Rate:             7.8 us (2X 85-95 C)
     Data Width:               64 bits
     SDRAM Width:              x8
     Voltage Interface:        1.5 V
     Max Case Temperature:     95 C (203 F)
     SPD Revision:             1.0
     Part Number:              9905402-015.A03LF
     Manufacturing Location:   China
     Manufacture Date:         September 2009 (0926h)
     Serial Number:            16CC37B4h
     Revision Code:            None
     EPP Support:              [ ]
     XMP Support:              [ ]

                  +-----------------------------------------+
                  |             Memory (SMBIOS)             |
                  +-----------------------------------------+
  Physical Memory Array 1
     Maximum Capacity:         16384 MB
     Location:                 System Board or Motherboard
     Use:                      System Memory
     Memory Error Correct.:    None
     Memory Devices:           4
     Structure Length:         0Fh
  Memory Device 1
     Size:                     1024 MB
     Form Factor:              DIMM
     Memory Type:              Unknown
     Speed:                    1333 MHz
     Device Locator:           A0
     Bank Locator:             Bank0/1
     Total Width:              64 bits
     Data Width:               64 bits
     Device Set:               00h
     Type Detail:              None
     Manufacturer:
     Serial Number:
     Asset Tag:
     Part Number:
     Structure Length:         1Bh
  Memory Device 2
     Size:                     1024 MB
     Form Factor:              DIMM
     Memory Type:              Unknown
     Speed:                    1333 MHz
     Device Locator:           A1
     Bank Locator:             Bank2/3
     Total Width:              64 bits
     Data Width:               64 bits
     Device Set:               00h
     Type Detail:              None
     Manufacturer:
     Serial Number:
     Asset Tag:
     Part Number:
     Structure Length:         1Bh
  Memory Device 3
     Size:                     Not Installed
     Form Factor:              DIMM
     Memory Type:              Unknown
     Speed:                    1333 MHz
     Device Locator:           A2
     Bank Locator:             Bank4/5
     Total Width:              64 bits
     Data Width:               64 bits
     Device Set:               00h
     Type Detail:              None
     Manufacturer:
     Serial Number:
     Asset Tag:
     Part Number:
     Structure Length:         1Bh
  Memory Device 4
     Size:                     Not Installed
     Form Factor:              DIMM
     Memory Type:              Unknown
     Speed:                    1333 MHz
     Device Locator:           A3
     Bank Locator:             Bank6/7
     Total Width:              64 bits
     Data Width:               64 bits
     Device Set:               00h
     Type Detail:              None
     Manufacturer:
     Serial Number:
     Asset Tag:
     Part Number:
     Structure Length:         1Bh

                  +-----------------------------------------+
                  |                   HDD                   |
                  +-----------------------------------------+
  Tertiary/Slave HDD
     HDD Model:                WDC WD1001FALS-00J7B0
     HDD Size:                 953869 MB (931.51 GB)
     Interface Type:           Serial ATA II
     Geometry:                 Heads: 16, Sectors: 63, Tracks: 16383
     Compatibility:            ATA/ATAPI-7
     Serial Number:            WD-WMATV0357962
     Controller Revision:      05.00K05
     HDD Marketing Size:       1000204 MB (1000.20 GB)
     Buffer Size:              32767.5 kB
     Buffer Type:              Not Specified
     HDD Temperature:          41 C (106 F)
     Reallocated Sectors:      0
     HDD Health Status:        Good
     ECC bytes:                50
     Security Erase Time:      194 min
     Enh. Security Erase:      194 min
     Current APM Value:        None
     Acoustic Management:      FEh (80h Recommended) - Disabled
     Access Method:            1
     ATA Controller Vendor:    ATI Technologies Inc
     ATA Controller Name:      SB700 SATA Controller [IDE mode]
     Device Location:          Tertiary/Slave
  Transfer Modes
     PIO Mode Support:         4
     SW DMA Mode Support:      Not Supported
     MW DMA Mode Support:      2, Active: None
     UDMA Mode Support:        6 (UltraDMA/133), Active: 6 (UltraDMA/133)
     Sectors per Interrupt:    16, Active: 16
  HDD Features
     SATA NCQ Command:                    [X]
     DMA Transfer:                        [X]
     LBA Supported:                       [X]
     Block Mode:                          [X]
     Double Word I/O:                     [ ]
     Standard Standby Timer:              [X]
     IORDY Supported:                     [X]
     IORDY may be Disabled:               [X]
     S.M.A.R.T.:                          [X] enabled
     S.M.A.R.T. Self-test:                [X] enabled
     S.M.A.R.T. Error Logging:            [X] enabled
     Security Mode Feature Set:           [X] disabled
     Removable Media:                     [ ]
     Power Management:                    [X] enabled
     PACKET Command:                      [ ]
     Write Cache:                         [X] enabled
     Look-ahead:                          [X] enabled
     Release Interrupt:                   [ ]
     Service Interrupt:                   [ ]
     Device Reset Command:                [ ]
     Host Protected Area:                 [X] enabled
     Write Verify Command:                [ ]
     Write Buffer Command:                [X] enabled
     Read Buffer Command:                 [X] enabled
     NOP Command:                         [X] enabled
     Identify Device DMA Command:         [ ]
     Download Microcode Command:          [X] enabled
     Read/Write DMA Queued:               [ ]
     CFA Feature Set:                     [ ]
     Advanced Power Management:           [ ]
     Removable Media Status:              [ ]
     Power-up in Standby:                 [X] disabled
     Set Features Req. to Spinup:         [X] enabled
     Set Max Security Extension:          [X] disabled
     Automatic Acoustic Management:       [X] disabled
     48-bit Address:                      [X] enabled
     Device Configuration Overlay:        [X] enabled
     Flush Cache Command:                 [X] enabled
     Flush Cache Ext Command:             [X] enabled
     Media Serial Number:                 [ ]
     Media Card Pass Through:             [ ]
     Streaming Feature Set:               [ ]
     General Purpose Logging:             [X] enabled
     Write DMA/Multiple FUA EXT:          [ ]
     Write DMA Queued FUA EXT:            [ ]
     World Wide Name:                     [X] enabled
  S.M.A.R.T.
     ID  | Attribute Name            |Threshold|Worst|Value| Raw Value
     ----+---------------------------+---------+-----+-----+-----------
     1   | Raw Read Error Rate       |       51|  200|  200|          0
     3   | Spin-up Time              |       21|  253|  253|       6066
     4   | Start/Stop Count          |        0|   96|   96|       4275
     5   | Reallocated Sectors Count |      140|  200|  200|          0
     7   | Seek Error Rate           |       51|  253|  100|          0
     9   | Power On Hours Count      |        0|   88|   88|       9391
     10  | Spin-up Retry Count       |       51|  100|  100|          0
     11  | Recalibration Retries     |       51|  100|  100|          0
     12  | Drive Power Cycle Count   |        0|   96|   96|       4251
     192 | Power-Off Retract Cycle   |        0|  199|  199|       1499
     193 | Load/Unload Cycle Count   |        0|  199|  199|       4275
     194 | Drive Temperature         |        0|   94|  109|         41
     196 | Reallocation Event Count  |        0|  200|  200|          0
     197 | Current Pending Sectors   |        0|  200|  200|          0
     198 | Uncorrectable Sectors     |        0|  200|  200|          0
     199 | UltraDMA CRC Error Rate   |        0|  200|  200|        267
     200 | Write Error Rate          |       51|  200|  200|          0
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard disk drives)
     Device Description:       Disk drive
     Friendly Name:            WDC WD1001FALS-00J7B0
     Device Class:             DiskDrive
     Device Location:          1
     Driver Provider:          Microsoft
     Driver Version:           5.1.2535.0
     Driver Date:              7-1-2001
     Inf File:                 disk.inf
     Service Name:             disk
     Hardware ID:              IDE\DiskWDC_WD1001FALS-00J7B0___________________05.00K05
     Compatible ID:            GenDisk

                  +-----------------------------------------+
                  |                  ATAPI                  |
                  +-----------------------------------------+
   ATAPI
     ATAPI Model:              _NEC DVD_RW ND-3550A
     ATAPI Type:               DVD+-RW DL/CD-RW
     Interface Type:           Parallel ATA
     Physical Interface:       ATAPI
     ATAPI Name:               _NEC DVD_RW ND-3550A
     Vendor Specific:          05093000
     CD Read Speed:            48x (Current: 48x)
     CD Write Speed:           48x (Current: 48x)
     DVD Read Speed:           Current: 6x
     DVD Write Speed:          Current: 6x
     Buffer Size:              2048 kB
     Loading Mechanism:        Tray Type
     Rotation Control:         CLV
     Read Retry Count:         15
     Write Retry Count:        0
     Compatibility:            Unknown
     Serial Number:            63E1J06S211
     Controller Revision:      1.05
     Command DRQ Type:         Microprocessor DRQ
     Command Packet Size:      12 bytes
     ATA Controller Vendor:    ATI Technologies Inc
     ATA Controller Name:      SB700 IDE
  Transfer Modes
     PIO Mode Support:         4
     SW DMA Mode Support:      Not Supported
     MW DMA Mode Support:      2, Active: None
     UDMA Mode Support:        2 (UltraDMA/33), Active: 2 (UltraDMA/33)
  Reading Features
     CD-R Disk Read:                      [X]
     CD-RW Disk Read:                     [X]
     DVD-ROM Disk Read:                   [X]
     DVD-RAM Disk Read:                   [ ]
     DVD-R Disk Read:                     [X]
     DVD-R DL Disk Read:                  [X]
     DVD-RW Disk Read:                    [X]
     DVD-RW DL Disk Read:                 [ ]
     DVD+R Disk Read:                     [X]
     DVD+R DL Disk Read:                  [X]
     DVD+RW Disk Read:                    [X]
     DVD+RW DL Disk Read:                 [ ]
     BD-ROM Disk Read:                    [ ]
     BD-R Disk Read:                      [ ]
     BD-RE Disk Read:                     [ ]
     HD DVD-ROM Disk Read:                [ ]
     HD DVD-RAM Disk Read:                [ ]
     HD DVD-R Disk Read:                  [ ]
     HD DVD-R DL Disk Read:               [ ]
     HD DVD-RW Disk Read:                 [ ]
     HD DVD-RW DL Disk Read:              [ ]
     Read Packet Using Method 2:          [X]
     Read Mode2 Form1 Sectors:            [X]
     Read Mode2 Form2 Sectors:            [X]
     Multisession Disk Read:              [X]
     READ-CD Command on AudioCD:          [X]
     Read Bar Code Capable:               [ ]
     Read Lead-in (CD-Text):              [X]
  Writing Features
     CD-R Disk Write:                     [X]
     CD-RW Disk Write:                    [X]
     DVD-RAM Disk Write:                  [ ]
     DVD-R Disk Write:                    [X]
     DVD-R DL Disk Write:                 [X]
     DVD-RW Disk Write:                   [X]
     DVD+R Disk Write:                    [X]
     DVD+R DL Disk Write:                 [X]
     DVD+RW Disk Write:                   [X]
     DVD+RW DL Disk Write:                [ ]
     BD-R Disk Write:                     [ ]
     BD-RE Disk Write:                    [ ]
     HD DVD-R Disk Write:                 [ ]
     HD DVD-R DL Disk Write:              [ ]
     HD DVD-RAM Disk Write:               [ ]
     HD DVD-RW Disk Write:                [ ]
     HD DVD-RW DL Disk Write:             [ ]
     Test Write Mode Support:             [X]
     Buffer Underrun Protection:          [X]
  Other Features
     Audio Play Support:                  [X]
     CD-DA Stream is Accurate:            [X]
     Composite Audio/Video:               [ ]
     Digital Output on Port 1:            [ ]
     Digital Output on Port 2:            [ ]
     Support Subcode R-W:                 [X]
     Support Subcode R-W D&C:             [ ]
     C2 Pointers Supported:               [X]
     ISRC Supported:                      [X]
     UPC Supported:                       [X]
  ATAPI Features
     DMA Transfer:                        [X]
     LBA Supported:                       [X]
     Block Mode:                          [ ]
     IORDY Supported:                     [X]
     IORDY may be Disabled:               [ ]
     ATA Software Reset:                  [ ]
     Overlap Operation:                   [ ]
     Command Queuing:                     [ ]
     Interleaving DMA:                    [ ]
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard CD-ROM drives)
     Device Description:       CD-ROM Drive
     Friendly Name:            _NEC DVD_RW ND-3550A
     Device Class:             CDROM
     Device Location:          0
     Driver Provider:          Microsoft
     Driver Version:           5.1.2535.0
     Driver Date:              7-1-2001
     Inf File:                 cdrom.inf
     Service Name:             cdrom
     Hardware ID:              IDE\CdRom_NEC_DVD_RW_ND-3550A____________________1.05____
     Compatible ID:            GenCdRom

   ATAPI
     ATAPI Model:              CD-W540E
     ATAPI Type:               CD-RW
     Interface Type:           Parallel ATA
     Physical Interface:       ATAPI
     ATAPI Name:               TEAC CD-W540E
     Vendor Specific:          09/30/02
     CD Read Speed:            48x (Current: 48x)
     CD Write Speed:           40x (Current: 40x)
     Buffer Size:              8192 kB
     Loading Mechanism:        Tray Type
     Rotation Control:         CLV
     Read Retry Count:         5
     Write Retry Count:        3
     Compatibility:            ATA/ATAPI-5 revision 19
     Serial Number:
     Controller Revision:      1.0H
     Command DRQ Type:         Accelerated DRQ
     Command Packet Size:      12 bytes
     ATA Controller Vendor:    ATI Technologies Inc
     ATA Controller Name:      SB700 IDE
  Transfer Modes
     PIO Mode Support:         4
     SW DMA Mode Support:      2, Active: None
     MW DMA Mode Support:      2, Active: None
     UDMA Mode Support:        2 (UltraDMA/33), Active: 2 (UltraDMA/33)
  Reading Features
     CD-R Disk Read:                      [X]
     CD-RW Disk Read:                     [X]
     DVD-ROM Disk Read:                   [ ]
     DVD-RAM Disk Read:                   [ ]
     DVD-R Disk Read:                     [ ]
     DVD-R DL Disk Read:                  [ ]
     DVD-RW Disk Read:                    [ ]
     DVD-RW DL Disk Read:                 [ ]
     DVD+R Disk Read:                     [ ]
     DVD+R DL Disk Read:                  [ ]
     DVD+RW Disk Read:                    [ ]
     DVD+RW DL Disk Read:                 [ ]
     BD-ROM Disk Read:                    [ ]
     BD-R Disk Read:                      [ ]
     BD-RE Disk Read:                     [ ]
     HD DVD-ROM Disk Read:                [ ]
     HD DVD-RAM Disk Read:                [ ]
     HD DVD-R Disk Read:                  [ ]
     HD DVD-R DL Disk Read:               [ ]
     HD DVD-RW Disk Read:                 [ ]
     HD DVD-RW DL Disk Read:              [ ]
     Read Packet Using Method 2:          [X]
     Read Mode2 Form1 Sectors:            [X]
     Read Mode2 Form2 Sectors:            [X]
     Multisession Disk Read:              [X]
     READ-CD Command on AudioCD:          [X]
     Read Bar Code Capable:               [ ]
     Read Lead-in (CD-Text):              [X]
  Writing Features
     CD-R Disk Write:                     [X]
     CD-RW Disk Write:                    [X]
     DVD-RAM Disk Write:                  [ ]
     DVD-R Disk Write:                    [ ]
     DVD-R DL Disk Write:                 [ ]
     DVD-RW Disk Write:                   [ ]
     DVD+R Disk Write:                    [ ]
     DVD+R DL Disk Write:                 [ ]
     DVD+RW Disk Write:                   [ ]
     DVD+RW DL Disk Write:                [ ]
     BD-R Disk Write:                     [ ]
     BD-RE Disk Write:                    [ ]
     HD DVD-R Disk Write:                 [ ]
     HD DVD-R DL Disk Write:              [ ]
     HD DVD-RAM Disk Write:               [ ]
     HD DVD-RW Disk Write:                [ ]
     HD DVD-RW DL Disk Write:             [ ]
     Test Write Mode Support:             [X]
     Buffer Underrun Protection:          [X]
  Other Features
     Audio Play Support:                  [X]
     CD-DA Stream is Accurate:            [X]
     Composite Audio/Video:               [ ]
     Digital Output on Port 1:            [ ]
     Digital Output on Port 2:            [ ]
     Support Subcode R-W:                 [X]
     Support Subcode R-W D&C:             [ ]
     C2 Pointers Supported:               [X]
     ISRC Supported:                      [X]
     UPC Supported:                       [X]
  ATAPI Features
     DMA Transfer:                        [X]
     LBA Supported:                       [X]
     Block Mode:                          [ ]
     IORDY Supported:                     [X]
     IORDY may be Disabled:               [X]
     ATA Software Reset:                  [ ]
     Overlap Operation:                   [ ]
     Command Queuing:                     [ ]
     Interleaving DMA:                    [ ]
     S.M.A.R.T.:                          [ ]
     S.M.A.R.T. Self-test:                [ ]
     S.M.A.R.T. Error Logging:            [ ]
     Security Mode Feature Set:           [ ]
     Removable Media:                     [ ]
     Power Management:                    [X] enabled
     PACKET Command:                      [X] enabled
     Write Cache:                         [ ]
     Look-ahead:                          [ ]
     Release Interrupt:                   [ ]
     Service Interrupt:                   [ ]
     Device Reset Command:                [X] enabled
     Host Protected Area:                 [ ]
     Write Verify Command:                [ ]
     Write Buffer Command:                [ ]
     Read Buffer Command:                 [ ]
     NOP Command:                         [X] enabled
     Identify Device DMA Command:         [ ]
     Download Microcode Command:          [ ]
     Read/Write DMA Queued:               [ ]
     CFA Feature Set:                     [ ]
     Advanced Power Management:           [ ]
     Removable Media Status:              [ ]
     Power-up in Standby:                 [ ]
     Set Features Req. to Spinup:         [ ]
     Set Max Security Extension:          [ ]
     Automatic Acoustic Management:       [ ]
     48-bit Address:                      [ ]
     Device Configuration Overlay:        [ ]
     Flush Cache Command:                 [ ]
     Flush Cache Ext Command:             [ ]
     Media Serial Number:                 [ ]
     Media Card Pass Through:             [ ]
     Streaming Feature Set:               [ ]
     General Purpose Logging:             [ ]
     Write DMA/Multiple FUA EXT:          [ ]
     Write DMA Queued FUA EXT:            [ ]
     World Wide Name:                     [ ]
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard CD-ROM drives)
     Device Description:       CD-ROM Drive
     Friendly Name:            TEAC CD-W540E
     Device Class:             CDROM
     Device Location:          1
     Driver Provider:          Microsoft
     Driver Version:           5.1.2535.0
     Driver Date:              7-1-2001
     Inf File:                 cdrom.inf
     Service Name:             cdrom
     Hardware ID:              IDE\CdRomTEAC_CD-W540E___________________________1.0H____
     Compatible ID:            GenCdRom

                  +-----------------------------------------+
                  |              Storage (ASPI)             |
                  +-----------------------------------------+
  Host: 0, Target: 1, LUN: 0
     Device Name:              Kingston DataTraveler II+
     Size:                     491 MB (0.48 GB)
     Device Type:              Disk Drive
     Compatibility:            Not Standard
     Vendor Specific:
     Serial Number:
     Controller Revision:      1.13
     HDD Marketing Size:       515 MB (0.51 GB)
     Location:                 Host: 0, Target: 1, LUN: 0
     Bus Width:                8-bit
     Address Width:            8-bit
  ASPI Device Features
     Removable Medium:                    Yes
     Read Cache:                          [ ]
     Write Cache:                         [ ]
     Read Reallocate:                     [ ]
     Write Reallocate:                    [ ]
     Terminate I/O Process:               [ ]
     Normal ACA:                          [ ]
     Hierarchical Support:                [ ]
     Embedded Array Controller:           [ ]
     Protection Information:              [ ]
     Enclosure Services:                  [ ]
     Multi-Ported Device:                 [ ]
     Medium Changer:                      [ ]
     Relative Addressing:                 [ ]
     Synchronous Transfer:                [ ]
     Linked Commands:                     [ ]
     Soft Reset:                          [ ]
     Quick Arbitration:                   [ ]
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard disk drives)
     Device Description:       Disk drive
     Friendly Name:            Kingston DataTraveler II+ USB Device
     Device Class:             DiskDrive
     Driver Provider:          Microsoft
     Driver Version:           5.1.2535.0
     Driver Date:              7-1-2001
     Inf File:                 disk.inf
     Service Name:             disk
     Hardware ID:              USBSTOR\DiskKingstonDataTraveler_II+1.13
     Compatible ID:            USBSTOR\Disk

                  +-----------------------------------------+
                  |              Logical Drives             |
                  +-----------------------------------------+
  Local Drives
  A:
     Drive Letter:             A:
     Drive Type:               Floppy 1.44 MB (3.5")
  C:[SYSTEM]
     Drive Letter:             C:
     Drive Type:               Fixed Disk
     Volume Label:             SYSTEM
     File System:              FAT
     Volume Serial Number:     2255-1BEA
     Total Size:               2047.0 MB
     Free Space:               787.8 MB (38.5%)
  D:[UTILITIES]
     Drive Letter:             D:
     Drive Type:               Fixed Disk
     Volume Label:             UTILITIES
     File System:              FAT
     Volume Serial Number:     2E4A-1BEB
     Total Size:               2047.1 MB
     Free Space:               16.7 MB (0.8%)
  E:[GAMES]
     Drive Letter:             E:
     Drive Type:               Fixed Disk
     Volume Label:             GAMES
     File System:              FAT
     Volume Serial Number:     2D54-1BEC
     Total Size:               2047.1 MB
     Free Space:               604.8 MB (29.5%)
  F:[INSTALL]
     Drive Letter:             F:
     Drive Type:               Fixed Disk
     Volume Label:             INSTALL
     File System:              FAT32
     Volume Serial Number:     146C-1611
     Total Size:               70.3 GB
     Free Space:               23.0 GB (32.7%)
  G:[MUSIC]
     Drive Letter:             G:
     Drive Type:               Fixed Disk
     Volume Label:             MUSIC
     File System:              NTFS
     Volume Serial Number:     D84A-C894
     Total Size:               815.2 GB
     Free Space:               29.1 GB (3.6%)
  H:[WINXP]
     Drive Letter:             H:
     Drive Type:               Fixed Disk
     Volume Label:             WINXP
     File System:              NTFS
     Volume Serial Number:     58B2-C918
     Total Size:               20.0 GB
     Free Space:               4.0 GB (20.0%)
  I:[VISTA]
     Drive Letter:             I:
     Drive Type:               Fixed Disk
     Volume Label:             VISTA
     File System:              NTFS
     Volume Serial Number:     84C7-F076
     Total Size:               20.0 GB
     Free Space:               1444.2 MB (7.1%)
  J:
     Drive Letter:             J:
     Drive Type:               Optical Drive
  K:
     Drive Letter:             K:
     Drive Type:               Optical Drive
  L:[KINGSTON]
     Drive Letter:             L:
     Drive Type:               Removable Disk
     Volume Label:             KINGSTON
     File System:              FAT
     Volume Serial Number:     94C6-CB33
     Total Size:               491.2 MB
     Free Space:               269.5 MB (54.9%)
  M:
     Drive Letter:             M:
     Drive Type:               Optical Drive

                  +-----------------------------------------+
                  |               USB Devices               |
                  +-----------------------------------------+
  USB Device 1
     Vendor (0951h):           Kingston Technology
     Device (1601h):           DataTraveler II Plus
     Manufacturer:             Kingston
     Product:                  DataTraveler II+
     Serial Number:            5B571621109C
     Device Version:           1.00
     Class (00h):              Unknown
     SubClass (00h):           Unknown
     Protocol (00h):           Unknown
     Configuration:
     USB Version:              2.00
     Speed:                    480 Mb/s
     Transfer Type:            Bulk
     Data Packet Size:         64 bytes
     Max Power:                200 mA
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             Compatible USB storage device
     Device Description:       USB Mass Storage Device
     Device Class:             USB
     Device Location:          DataTraveler II+
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.0
     Driver Date:              7-1-2001
     Inf File:                 usbstor.inf
     Service Name:             USBSTOR
     Hardware ID:              USB\Vid_0951&Pid_1601&Rev_0100
     Compatible ID:            USB\Class_08&SubClass_06&Prot_50
  Interface 1
     Class (08h):              Mass Storage
     SubClass (06h):           SCSI
     Protocol (50h):           Bulk (Zip)
     Interface:

  USB Device 2
     Vendor (046Dh):           Logitech
     Device (C05Ah):           USB Optical Mouse
     Manufacturer:             Logitech
     Product:                  USB Optical Mouse
     Serial Number:
     Device Version:           54.00
     Class (00h):              Unknown
     SubClass (00h):           Unknown
     Protocol (00h):           Unknown
     Configuration:
     USB Version:              2.00
     Speed:                    480 Mb/s
     Transfer Type:            Interrupt
     Data Packet Size:         8 bytes
     Max Power:                98 mA Remote Wakeup
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       USB Human Interface Device
     Device Class:             HIDClass
     Device Location:          USB Optical Mouse
     Driver Provider:          Microsoft
     Driver Version:           5.1.2600.2180
     Driver Date:              7-1-2001
     Inf File:                 input.inf
     Service Name:             HidUsb
     Hardware ID:              USB\Vid_046d&Pid_c05a&Rev_5400
     Compatible ID:            USB\Class_03&SubClass_01&Prot_02
  Interface 1
     Class (03h):              Human Interface Devices
     SubClass (01h):           Boot Interface Subclass
     Protocol (02h):           Mouse
     Interface:

                  +-----------------------------------------+
                  |            Physical Printers            |
                  +-----------------------------------------+
     LPT/PnP or USB printer not found

                  +-----------------------------------------+
                  |              Slots (SMBIOS)             |
                  +-----------------------------------------+
  Slot PCI
     Slot Type:                PCI
     Current Usage:            Available
     Data Bus Width:           32 bit
     Slot Designation:         PCI
     Slot Length:              Long Length
     Slot ID:                  7
  Slot PCI
     Slot Type:                PCI
     Current Usage:            In Use
     Data Bus Width:           32 bit
     Slot Designation:         PCI
     Slot Length:              Long Length
     Slot ID:                  6
  Slot PCI Express
     Slot Type:                PCI Express
     Current Usage:            Unknown
     Data Bus Width:           16x or x16
     Slot Designation:         PCI Express x16
     Slot Length:              Other
     Slot ID:                  0

                  +-----------------------------------------+
                  |              Ports (SMBIOS)             |
                  +-----------------------------------------+
  Port 1 Other
     Int. Connector Type:      On Board IDE
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          PRIMARY IDE
     Ext. Designator:
  Port 2 8251 FIFO Compatible
     Int. Connector Type:      On Board Floppy
     Ext. Connector Type:      None
     Port Type:                8251 FIFO Compatible
     Int. Designator:          FDD
     Ext. Designator:
  Port 3 Serial Port 16450 Compatible
     Int. Connector Type:      9 Pin Dual Inline (pin 10 cut)
     Ext. Connector Type:      DB-9 pin male
     Port Type:                Serial Port 16450 Compatible
     Int. Designator:          COM1
     Ext. Designator:
  Port 4 Serial Port 16450 Compatible
     Int. Connector Type:      9 Pin Dual Inline (pin 10 cut)
     Ext. Connector Type:      DB-9 pin male
     Port Type:                Serial Port 16450 Compatible
     Int. Designator:          COM2
     Ext. Designator:
  Port 5 Parallel Port ECP/EPP
     Int. Connector Type:      DB-25 pin female
     Ext. Connector Type:      DB-25 pin female
     Port Type:                Parallel Port ECP/EPP
     Int. Designator:          LPT1
     Ext. Designator:
  Port 6 Keyboard Port
     Int. Connector Type:      Other
     Ext. Connector Type:      PS/2
     Port Type:                Keyboard Port
     Int. Designator:          Keyboard
     Ext. Designator:
  Port 7 Mouse Port
     Int. Connector Type:      PS/2
     Ext. Connector Type:      PS/2
     Port Type:                Mouse Port
     Int. Designator:          PS/2 Mouse
     Ext. Designator:          No Detected
  Port 8 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 9 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 10 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 11 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 12 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 13 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 14 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 15 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 16 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 17 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 18 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 19 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:

                  +-----------------------------------------+
                  |                 Network                 |
                  +-----------------------------------------+
  Network
     Network Name:             A2KKV_XP
     User Name:                kkv1
     User Role:                Administrator
     Logon Domain:             A2KKV_XP
  Interface 1
     Description:              TAP-Win32 Adapter V8 - Packet Scheduler Miniport
     MAC Address:              00-FF-0C-27-A1-46
     Adapter Type:             Ethernet
     Link Speed:               10.0 Mbps
     MTU Size:                 1500 byte
     Adapter Status:           Enabled
     Operational Status:       Non Operational
     DHCP Server:              192.168.101.2
  Interface 2
     Adapter Vendor:           Realtek Semiconductor
     Adapter Name:             RTL8168/8111 PCI-E Gigabit Ethernet NIC
     Subsys Vendor:            Giga-Byte Technology
     Subsystem ID:             GA-EP45-DS5 Motherboard
     Bus Type:                 PCI-E
     Description:              Realtek RTL8168C(P)/8111C(P) PCI-E Gigabit Ethernet NIC - Packet Scheduler Miniport
     MAC Address:              00-24-1D-89-15-40
     Adapter Type:             Ethernet
     Link Speed:               100.0 Mbps
     MTU Size:                 1500 byte
     Adapter Status:           Enabled
     Operational Status:       Operational
     DHCP Server:              192.168.1.1
     IP Address:               192.168.1.141
     IP Address Subnet Mask:   255.255.255.0
     Gateway:                  192.168.1.1
     DNS Server:               192.168.1.1

                  +-----------------------------------------+
                  |                 Monitor                 |
                  +-----------------------------------------+
  Monitor
     Monitor Vendor:           LG Electronics Inc.
     Monitor Model:            LG FLATRON F920P
     Viewable Size:            17.7" (45.0 sm)
     Serial Number:            319823
     Manufacture Date:         March 2005
     EDID Version:             1.3
     Monitor ID:               GSM4A88
     Aspect Ratio:             4:3
     Horizontal Size:          36 sm
     Vertical Size:            27 sm
     Gamma Factor:             2.910
     Display Type:             RGB Color
     Input Signal:             Analog
     Internal Model:           F920P
     Vertical Frequency:       50-160 Hz
     Horizontal Frequency:     30-111 kHz
  DPMS Features
     Active Off:               [X]
     Suspend:                  [X]
     Standby:                  [X]
  Supported Modes
     Mode 1:                   720x400   @ 70 Hz (VGA)
     Mode 2:                   720x400   @ 88 Hz (XGA2)
     Mode 3:                   640x480   @ 60 Hz (VGA)
     Mode 4:                   640x480   @ 67 Hz (Mac II)
     Mode 5:                   640x480   @ 72 Hz (VESA)
     Mode 6:                   640x480   @ 75 Hz (VESA)
     Mode 7:                   800x600   @ 56 Hz (VESA)
     Mode 8:                   800x600   @ 60 Hz (VESA)
     Mode 9:                   800x600   @ 72 Hz (VESA)
     Mode 10:                  800x600   @ 75 Hz (VESA)
     Mode 11:                  832x624   @ 75 Hz (Mac II)
     Mode 12:                  1024x768  @ 87 Hz (interlaced)
     Mode 13:                  1024x768  @ 60 Hz (VESA)
     Mode 14:                  1024x768  @ 70 Hz (VESA)
     Mode 15:                  1024x768  @ 75 Hz (VESA)
     Mode 16:                  1280x1024 @ 75 Hz (VESA)
     Mode 17:                  1920x1440 @ 70 Hz
     Mode 18:                  2048x1536 @ 60 Hz
     Mode 19:                  1024x768  @ 85 Hz
     Mode 20:                  1280x1024 @ 75 Hz
     Mode 21:                  1280x1024 @ 85 Hz
     Mode 22:                  1600x1200 @ 75 Hz
     Mode 23:                  1600x1200 @ 85 Hz
     Mode 24:                  1152x864  @ 75 Hz
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             LG
     Device Description:       F920P
     Device Class:             Monitor
     Driver Provider:          LG
     Driver Version:           1.0.0.0
     Driver Date:              5-4-2004
     Inf File:                 oem8.inf
     Hardware ID:              Monitor\GSM4A88
     Compatible ID:            *PNP09FF

                  +-----------------------------------------+
                  |                  Video                  |
                  +-----------------------------------------+
  Video
     Video Chip Vendor:        ATI Technologies Inc
     Video Chip:               RV770 [Radeon HD 4870]
     Subsystem Vendor:         Hightech Information System Ltd (Medion??)
     Video Memory Size:        512 MB
     Video BIOS Date:          01/05/09
     Bus Type:                 PCI-E
  PCI-E Capabilities
     PCI Express Version:      2
     Link Speed:               5.0 GB/s (Current: 5.0 GB/s)
     Link Width:               x16 (Current: x16)
     Link Port Number:         0
     Physical Slot Number:     0
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             ATI Technologies Inc.
     Device Description:       ATI Radeon HD 4800 Series
     Device Class:             Display
     Device Location:          PCI bus 1, device 0, function 0
     Driver Provider:          ATI Technologies Inc.
     Driver Version:           8.753.0.0
     Driver Date:              7-6-2010
     Inf File:                 oem7.inf
     Service Name:             ati2mtag
     Hardware ID:              PCI\VEN_1002&DEV_9440&SUBSYS_22671787&REV_00
     Compatible ID:            PCI\VEN_1002&DEV_9440&REV_00

                  +-----------------------------------------+
                  |          Drivers Troubleshooter         |
                  +-----------------------------------------+
  List of Problem Devices
  Problem Device 1
     Device Type:              PCI/AGP Device
     Vendor (1102h):           Creative Labs
     Device (0004h):           EMU10K2 Audio Chipset (SB Audigy Series)
     Subsys Vendor (1102h):    Creative Labs
     Subsystem ID (2005h):     Unknown
     Class (04h):              Multimedia
     SubClass (01h):           Audio
     Revision:                 04h
     Driver Status:            The device is disabled (22)
     Manufacturer:             Creative Technology, Ltd.
     Device Description:       Creative Audigy Audio Processor (WDM)
     Friendly Name:            Creative SB Audigy 2 ZS (WDM)
     Device Class:             MEDIA
     Device Location:          PCI bus 3, device 6, function 0
     Driver Provider:          Creative
     Driver Version:           5.12.8.1164
     Driver Date:              12-8-2005
     Inf File:                 oem9.inf
     Service Name:             ctaud2k
     Hardware ID:              PCI\VEN_1102&DEV_0004&SUBSYS_20051102&REV_04
     Compatible ID:            PCI\VEN_1102&DEV_0004&REV_04

                  +-----------------------------------------+
                  |             HDD Diagnostics             |
                  +-----------------------------------------+
  HDD 1 Status
     HDD Model:                WDC WD1001FALS-00J7B0
     HDD Size:                 953869 MB (931.51 GB)
     Interface Type:           Serial ATA II
     Serial Number:            WD-WMATV0357962
     Controller Revision:      05.00K05
     HDD Marketing Size:       1000204 MB (1000.20 GB)
     Buffer Size:              32767.5 kB
     ATA Controller Vendor:    ATI Technologies Inc
     ATA Controller Name:      SB700 SATA Controller [IDE mode]
     Device Location:          Tertiary/Slave
     HDD Temperature:          41 C (106 F)
     Reallocated Sectors:      0
     HDD Health Status:        Good

                  +-----------------------------------------+
                  |                 Windows                 |
                  +-----------------------------------------+
  Windows
     Operating System:         MS Windows XP Professional (5.1.2600 Service Pack 2)
     OS Language:              English (United States)
     Windows Folder:           H:\WINDOWS
     Installation Date:        August 23, 2010
     Kernel Type:              Multiprocessor Free
     Licensed Processors:      2
     Registered Owner:         -
     Registered Organization:  -
     Product ID:               55274-647-9588401-23057
     System UpTime:            0 Hour(s) 3 Minutes 7 Seconds
     IE Version:               Internet Explorer 6 for Windows XP SP2 (6.0.2900.2180)
     DirectX Version:          DirectX 9.0c (4.09.00.0904)
  Regional Settings
     Country:                  Russia
     Language:                 Russian
     Time Zone:                Caucasus Standard Time (GMT+4)
     Currency Name:            Russian Ruble
     Measurment System:        Metric
     ANSI Code Page:           1251
     OEM Code Page:            866

                  +-----------------------------------------+
                  |            Installed Programs           |
                  +-----------------------------------------+
  Installed Programs
     Sysinfo Lab ASTRA32 - Advanced System Information Tool 2.11
     AMD Processor Driver v1.3.2.0053
     Realtek REALTEK GbE & FE Ethernet PCI-E NIC Driver v1.20.0000
     Realtek Semiconductor Corp. Realtek High Definition Audio Driver v5.10.0.5780

                  +-----------------------------------------+
                  |            Installed Hotfixes           |
                  +-----------------------------------------+
  Installed Hotfixes
     Microsoft Corporation High Definition Audio Driver Package - KB888111 v20040219.000000

                                [End of Report]
