================================================================================
Realtek Driver for Windows 98/NT           version 4.00
================================================================================
Windows 98
----------
========================
Realtek8139 Method
------------------------------------------------------
1 Start Microsoft Windows 98.

2 Click the Start button, point to Settings, and click Control Panel.

3 Right-click My Computer, and click the properties tab.

4 Click Other devices tab, then click PCI Ethernet controller Device.

5 Click Driver tab,click update driver tab.then show update Device Driver Wizard, click Next.

6 Choice search for a better driver than one your device is using now(Recommender).

7 point specify a location,click Browse,example D:\Network\Rtl8139\Exe\Win98\Netrts5.inf,Click Next
 
8 Click  Finish . 

10 It is last, It want to insert Win98 CD to install.  
****************************************************************************
            Realtek8139 PCI Fast Ethernet Adapter Installation
                   for Windows NT 4.0 Driver
****************************************************************************



To install the Realtek PCI Fast Ethernet adapter and driver for use with
Windows NT 4.0, please do the following:

1.  Power off your PC and install the adapter in a PCI slot in your PC.

2.  Reboot the computer using the Windows NT operating system.

3.  Double click the Network icon in the Control Panel.

4.  Select the "Adapter" tab and click "Add..."

5.  Select Have Disk. Insert the "Mainboard Utility CD Disk" in your CD-ROM drive
    and specify the correct path (D:\Network\RTL8139\EXE\Winnt4).

6.  Select one of the following models:

    "Realtek RTL8139/810x Family PCI Fast Ethernet Adapter"

    then click OK.

7.  In the dialog box that appears, select the Media Type and enter the
    Network address for the adapter if necessary(You can click Help for more
    detailed information about these settings).
    Click OK to complete this dialog box (or Cancel to terminate the
    configuration without completing it).

8.  Exit the Network control panel window. Windows NT asks if you wish to
    reboot. You must reboot before the adapter will function properly.

