(C)Copyright 2003-2006 Marvell(R).
All rights reserved.
==========================================================

SetupYukonWin.txt created 06-Jun-2006

Readme File for SETUPYUKONWIN.exe v8.56.2.3

Supporting: Marvell Yukon Ethernet Controller

Operating Systems:
Windows 98 SE, Windows Me, Windows NT 4.0, Windows 2000,
Windows XP, Windows Server 2003




This file contains
 1  Overview
 2  Required File
 3  Installation
 4  Silent Installation
    4.1  Driver Installation
    4.2  Driver Removal
    4.3  Driver Repair
    4.4  Further Options
 5  Troubleshooting


==========================================================


1  Overview
===========


The driver installation package contains the Marvell NDIS
Miniport Driver for the Marvell Yukon Ethernet Controller.

This README file explains how to install the driver
installation package on a machine running one of the
following operating systems:

Windows 98 SE, Windows Me, Windows NT 4.0, Windows 2000,
Windows XP, Windows Server 2003



2  Required File
================


To install the driver, the following file is required:

    SetupYukonWin.exe



3  Installation
===============


On plug & play Windows versions the adapter is found,
identified and configured automatically. Cancel all
operating system attempts to install the driver
automatically.

NOTE: To install the driver you have to be logged in as 
      a user with administrative rights.

To install the driver, proceed as follows:

1. Execute the setup file "SetupYukonWin.exe".
2. Follow the instructions displayed during the 
   installation procedure.



4  Silent Installation
======================


NOTE: Silent installation is not supported for 
      Windows NT 4.0. 

In order to install the driver silently the following
commands should be executed.

4.1  Driver Installation
------------------------

SetupYukonWin.exe /S /V"/LIME %WINDIR%\YukonInstall.log
REBOOT=ReallySuppress /qn"


4.2  Driver Removal
-------------------

SetupYukonWin.exe /S /V"/LIME %WINDIR%\YukonInstall.log
REMOVE=ALL REBOOT=ReallySuppress /qn"


4.3  Driver Repair
------------------

SetupYukonWin.exe /S /V"/LIME %WINDIR%\YukonInstall.log
REINSTALLMODE=vomus REINSTALL=ALL REBOOT=ReallySuppress
/qn"

NOTE: On Windows 98 SE and Windows Me it is recommended 
      to use "REBOOT=Force" instead of 
      "REBOOT=ReallySupress" because each driver 
      installation needs a reboot for completion.


4.4  Further Options
--------------------

By default the installation directory is
"%PROGRAMFILES%\Marvell\Miniport Driver". It can be changed
by setting the variable "INSTALLDIR".

Example :

SetupYukonWin.exe /S /V"/LIME %WINDIR%\YukonInstall.log
INSTALLDIR=C:\MyDir REBOOT=ReallySuppress /qn"

The installation status is logged in the file
"%WINDIR%\YukonInstall.log". The log file path and name can
be changed by replacing "%WINDIR%\YukonInstall.log" with
the preferred file path and name.



5  Troubleshooting
==================


If you should encounter any problems with your driver
installation package, please re-read the instructions above
and the documentation supplied with the operating system
carefully.

Additionally refer to your system event log file (using the
Event Viewer) and check it for entries from the Marvell
NDIS Miniport Driver. If your particular problem is not
listed or the error persists, please send your system event
log file to our technical support.

For further information please contact our support.


*** End of Readme File ***


