SiS191/190 10/100/1000Mbs adapter manufacture test tools package release note

======
v2.02
======
1. Initial release.

======
v2.03
======
1. Modify the naming of executive file to indicate it is used for SiS191/190 
   only. ex. lan19x.exe
2. Add the needed file "MODERN.FON" while executing exlb19x.exe. 
3. Fix the issue fail to run Diag.exe.  

======
v2.04
======
1. DIAG19x.exe: Fix the problem of internal loopback test fail that happened 
   after external loopback test in half duplex mode. 

======
v2.05
======
1. DIAG19x.exe: Rx got packet when external loopback test failed in half duplex mode. 
2. DIAG19x.exe: Fix the issue that internal loopback test fails sometimes.

======
v2.06
======
1. DIAG19x.exe: Fix 2 station test package lose issue.

======
v2.09
======
1. DIAG19x.exe: Fix the issue that Node ID cannot be read.
2. DIAG19x.exe: Fix the issue of Tx error for Diag19x 100/Full internal loopback test.
3. DIAG19x.exe: Fix the issue of failure for MII and PCI registers test.
4. DIAG19x.exe: It is ready for Broadcom AC131 and Marvell 88e1111 PHY.

======
v2.10
======
1. Realtek RTL8211 PHY is supported.
2. Add 1000 Mbps external loopback test for RTL8211 PHY.

======
v2.11
======
1. Fix the issue that exlb19x can't set font.

======
v2.12
======
1. ee19x.exe can support 190/191 EEPROM signature auto recognization.

======
v2.13
======
1. Fix the halt issue on SiS656 & SiS649.

======
v2.14
======
1. Support SiS191 REV.01 on SiS966.
2. Support Marvell PHY new chip (PHY ID: 0x01410cc2)
3. Support RGMII mode.

======
v2.15
======
1. Fix the failuration of Agere MII register test. 

======
v2.16
======
1. Fix the conflict between PCI register test and USB Legacy support.
